Vicon® Industries Inc		VLR-XTBVX NETWORK RECORDING SERVERS	 VALERUS® SYSTEM	 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE
PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components, regularly manufactured, 
regularly utilized in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24-hour 
immediate technical assistance for either the dealer/installer at no charge.

D.	All systems and components shall be provided with an explicit manufacturer warranty.

2.02	DIGITAL SERVERS 

A.	The digital application server and recording server (NVR) shall be a PC computer with a Microsoft® Windows® 10 LTSB* (64-bit) operating system. It shall be fully equipped with the Digital Video Management Software. It shall require an external monitor, keyboard and mouse for operation. A mini recording server shall also be available.

B.	As a minimum, the server shall have Intel® Core™ i5 processor; the mini version shall have an Intel® Core™ i3 processor. It shall have a minimum of 8 GB of RAM memory, USB ports, and monitor outputs. 

C.	The server shall be housed in a desktop or rack-mount case with all suitable connectors available on the back panel**. It shall be constructed of steel and plastic materials. It shall also be operated indoors in a temperature range not to exceed 32 to 104° F (0 to 40° C) and a humidity range not to exceed 0 to 95% relative, in a non-condensing atmosphere. The server shall employ a Universal Voltage Power Supply requiring 105 - 240 VAC @ 50 - 60 Hz. A rack-mounting bracket kit shall be provided.

*A full windows O.S. is available on request. **The desktop and 1U rack-mount versions support up to a certain drive size. Larger drive capacity is available, but may require a larger tower or 2U chassis. Contact your sales representative.

D.	The recording server shall offer internal hard-drive storage with the following capacities:
1.	1 TB.
2.	2 TB.
3.	3 TB.
4.	4 TB.
5.	6 TB.
6.	8 TB
7.	10 TB
8.	12 TB
9.	14 TB
10.	16 TB

E.	The application server can be a standalone unit with no storage capability or an all-in-one unit included in the recording server.

F.	The mini recording server shall offer internal hard-drive storage with the following capacities:
1.	1 TB.
2.	2 TB.
3.	3 TB.
4.	4 TB.
5.	6 TB.
6.	8 TB

G.	A client viewing station shall be available with 2 or 4 monitor outputs.

H.	A model shall be available with internal RAID storage, 8-bay and 24-bay models. These shall be available in the following capacities (RAID 5; available in RAID 6 with slightly lower storage capacities): 
1.	6.5 TB.
2.	13 TB.
3.	17 TB.
4.	22 TB.
5.	38 TB.
6.	57 TB
7.	95 TB
8.	114 TB
9.	152 TB
I.	
J.	The servers shall be preloaded with Valerus Video Management Software.     
2.03	
ELECTRICAL SPECIFICATIONS 

A.		Input Voltage:	105-240 ±10% VAC, 50/60 Hz.	
B.		Current:	0.66 A @ 115VAC; 0.33 A @ 240 VAC.
8-bay internal storage: 1.5 A @ 115VAC; 0.75A @ 240 VAC.
24-bay internal storage: 8.8 A @ 115VAC; 4.4A @ 240 VAC.	
C.		Power Consumption:  	
76 W.
8-bay internal storage: 178 W.
24-bay internal storage: 1010 W; includes redundant power supply.	
D.		CPU	Intel® Core™ i5.	
E.		RAM Memory	8 GB minimum.	
F.		Heat Output:  	266 btu/hour.	
G.		Storage:	1 TB to 16 TB. Depending on model.	
H.		Operating System:	Microsoft Windows 10 LTSB.	
I.		LAN Interface:	100/1000 Base T Ethernet interface on main board.	
J.		Front Panel
Controls/Indicators:	
Power, network activity LEDs, USBs.	
K.		Certifications:	UL, FCC Class A, CE.	

2.04	MECHANICAL SPECIFICATIONS 

A.		Application:	Indoor.	
B.		Mounting:	ITX-mini desktop, mini desktop or rack unit mounted in a standard EIA compliant rack, 19 in. (483 mm) wide opening. Rack height is 1.75 in. (44 mm) or 1 RU.	
C.		Dimensions-Rack:  	Width (W): 19.0 in. (483 mm).
Depth (D): 16 in. (406mm).
Height (H): 1.75 in. (44.45 mm), 1 RU.
8-bay internal storage: Width (W): 19 in. (483 mm).
         Depth (D): 26 in. (660 mm).
         Height (H): 3.5 in. (89 mm).
24-bay internal storage: Width (W): 19 in. (483 mm).
         Depth (D): 28 in. (711 mm).
         Height (H): 7 in. (176 mm).	
D.		Dimensions-Desktop	ITX: Width (W): 2.13 in. (44 mm).
        Depth (D): 6.59 in. (167.5 mm).
        Height (H): 6.59 in. (167.5 mm).
Mini: Width (W): 7.9 in. (200 mm).
         Depth (D): 7.5 in. (200 mm).
         Height (H): 3.15 in. (80 mm).	
E.		Weight-Rack:	18.2 lb. (8.3 kg) approximately.
8-bay internal storage: 46.3 lb (21 kg).
24-bay internal storage: 64.0 lb (29 kg).	
F.		Weight- Desktop:	8.1 lb. (3.7 kg) approximately.	
G.		Construction:	Steel and plastic.	
H.		Color:	Black.	

2.05	ENVIRONMENTAL SPECIFICATIONS 

A.	Operating 
Temperature Range:	
32 to 104ºF (0 to 40ºC).	
B.	Operating 
Humidity Range:	
0 to 95%, non-condensing.	

2.06	CERTIFICATIONS

A.	UL
B.	CE
C.	FCC, Class A

2.07	WARRANTY

A.	3 years, parts and labor 

2.08	APPROVED MANUFACTURERS

A.	The Video Management System shall be Vicon’s Valerus. The Application Server shall be models VLR-APPSRV (desk-top) and VLR-APPSRV-RK (rack-mount). The Recording Server shall be models VLR-XTBV1 (preloaded desk-top) and VLR-XTBV1-RK (preloaded rack-mount). The models with internal RAID shall be VLR-XTBV1-R5. The mini server shall be model VLR-MINI-XTBV1. (X is the hard drive size). The Viewing Station shall be VLR-CLIENT/VLR-CLIENT-4 (desk-top; 2 or 4 monitor) and VLR-CLIENT-RK/VLR-CLIENT-4-RK (rack-mount; 2 or 4 monitor).

END OF SECTION

Vicon and Vicon Valerus are registered trademarks or trademarks of Vicon Industries, Inc in the United States and other countries.
Microsoft and Microsoft Windows, are registered trademarks of Microsoft Corporation in the United States and other countries.
Intel and Core are trademarks or registered trademarks of Intel Corporation.