Vicon® Industries IQEYE 9 SERIES BOX CAMERA
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	IP BOX CAMERA 

A.	The indoor box camera shall be available without a lens or incorporate a camera/lens combination; a motorized varifocal lens shall be available as well as a model with no lens which will accept a CS-mount lens. The high-resolution day/night camera shall be available with an integral 2.8-12 or 2.8-8.5 mm motorized zoom and focus varifocal lens. Day/night operation shall be achieved using a built-in IR-cut filter. Wide Dynamic Range (WDR) shall be available on the 1 MP and 2 MP models.

B.	The box camera shall be powered by PoE, 24 VAC or 12 VDC. 

C.	The box camera shall have simultaneous dual streaming video and support H.264 and M-JPEG compression. The camera shall be available in 4 resolutions, 1 MP (720p), 2 MP (1080p), 3.1 MP and 5 MP.

D.	Two-way audio shall be available as well as an on-camera microphone. Alarm I/O relay shall be available as well as analog video out.

E.	Camera features shall include AGC, BLC, white balance, automatic exposure, electronic shutter, flip and rotate 180°, privacy masks, and motion detection.

F.	The box camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF interface and PSIA. 

G.	The box camera shall provide a slot for an SD card for local storage.

H.	The box camera shall meet or exceed the following design and performance specifications.

2.03	
DAY/NIGHT IP BOX CAMERA SPECIFICATIONS

A.	Imaging Device:	1/2.7-inch (1MP and 2MP)1/3.2-inch (3MP and 5MP)
B.	Max. Resolution:	1 megapixel (720p); 2 megapixel (1080p), 3.1 megapixel 
	and 5 megapixel models
C.	Shutter Speed:	Auto/Programmable/Fixed
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity:	Color: 1-2 MP: 0.1 lux; 3-5 MP: 0.2 lux; 
B&W: <0.05 lux 
F.	Tilt and Horizontal	Dependent on mount
G.	Lens Adjustment:	Motorized zoom and focus and P-iris
H.	Focal Length:	2.8-12 mm or 2.8-8.5 mm varifocal
I.	Horizontal Field of View:	2.8-12 mm: 101°- 35°; 2.8-8.5 mm 93°- 44° 

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	PoE; 12 VDC; 24 VAC
B.	Power Consumption:	<4 W
C.	Connectors:	Power: PoE RJ-45 
		Video/Data: RJ-45
		Push-in terminal for I/O relay; audio in/out; analog output
		Slot for SD card
D.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	32° to 113°F (0° to 45°C) 

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum and plastic
B.	Dimensions:	Height: 2.76 in. (70.2 mm), 
Width: 2.72 in. (69)
Length: 5.07 in. (128.9 mm))
C.	Weight: 	Approximately 0.4 lb (0.165 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	¼-20 mounting holes, top and bottom 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with ViconNet Digital Video
                                              Management System 
B.	Compression:	H.264; MPEG-4; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Multicast
D.	Video Channels	Dual streaming
E.	Max. Resolution/Frame Rate: 720p: 1280x720
   1080p: 1920x1080
   3.1 MP: 2048x1536
   5 MP: 2560x1920
1, 2, MP: 30 fps; 3.1 MP: 20 fps; 5 MP: 10 fps
F.	Web Browser:	Internet Explorer, Firefox, Chrome, Safari, Mozilla, 
	Opera
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Auto exposure; configurable brightness, contrast, 
	saturation, and sharpness; auto white balance, AGC; 
	BLC; motion detection; AC lighting control (50 or 60 Hz)
I.	Supported Protocols:	IPV4, IPV6 (available with firmware update) TCP, HTTP, 
                                             HTTPS, RTSP, RTP, CIFS, SMTP, DHCP, NTP, DNS, 
                                             UDP, uPnP, ARP, SNMP, ICMP, Zeroconf, APIPA, 
                                             Telnet, multicast 

2.09	CERTIFICATIONS

A.	CE
B.	FCC, Class A
C.	UL/cUL
D.	RoHS 2
E.	ONVIF
F.	PSIA

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The IP box camera shall be Vicon Industries Models IQB91WI-A5, IQB92WI-A5, IQB93NI-NL, IQB93NI-A6, IQB95NI-NL and IQB95NI-A6. Models with A5 and A6 have a motorized varifocal lens.
B.	An IR accessory shall be available, model IQB9-IR. A PoE housing shall be available, model HPOE-100.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.