Vicon® Industries SN683D-WIR NETWORK PTZ DOME
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

D.	All systems and components shall be provided with an explicit 3-year manufacturer warranty.

2.02	NETWORK CAMERA DOME FEATURES

A.	The compact network dome shall be comprised of a camera/lens and pan/tilt drive in an attractive covert enclosure. It shall be have 3 MP resolution.

B.	The network dome shall be shall provide network video transmission using either open platform H.265/H.264 or M-JPEG compression. The dome shall support ONVIF open architecture connectivity to enable third party software recording. The camera dome shall transmit high quality video across the network for remote viewing and recording and shall be configurable remotely from network digital video recorders and master workstations

C.	Four alarm inputs shall be programmable for functional state (enabled or disabled); it shall be able to be set for Normally Open (NO) or Normally Closed (NC) and a dwell time shall be programmable from 1-180 second. The alarm output shall be able to control external equipment; it shall be able to be set for Normally Open (NO) or Normally Closed (NC). An audio alert shall be available.

D.	There shall be 256 individual programmable preset positions available. Each preset shall be able to have an individual title and shall be adjustable for pan and tilt speed and manual or auto focus.

E.	There shall be eight tours available with up to 64 presets per tour. Each tour shall be able to have an individual title and shall be adjustable for pan, tilt and zoom speed and dwell time. Tours shall be able to be programmed to repeat.

F.	Pan and tilt functions shall be programmable. Maximum manual pan and tilt speeds shall be programmable. Maximum pan speed shall be 380 degrees/sec and maximum tilt speed shall be 380 degrees/sec. Pan and tilt speeds shall also be scalable to the zoom setting. The pan range shall be 360 degree continuous and tilt range shall be 100 degrees (-10 to 90 degrees).

G.	The camera/lens shall be 3 MP 1/2.8-in. progressive scan CMOS true day/night (IR cut filter) with a 4.6-165 mm varifocal lens (optical 36x). The camera shall feature true wide dynamic range (120 dB) to provide the highest quality image with excellent contrast.

H.	 The camera shall provide synchronized IR illuminators with 1312 ft (400 m) range.

I.	The camera shall provide high level, programmable functions. Configuration of the dome shall be done through a web browser. There shall be a dynamic adjustable bit rate. Brightness, sharpness and high-sensitivity shall be configurable. The gain control shall be adjustable. The shutter speed shall be programmable, automatic or manual. The camera shall have white balance gain using red and blue scales. Backlight compensation or Wide Dynamic Range shall be programmable. Horizontal flip shall be available. There shall be Dynamic Noise Reduction control. Video Content Analysis (VCA) shall be provided for tampering, defog, digital image stabilization, face detection, line detector and field detector.

J.	The rugged PTZ housing shall be constructed of die-cast aluminum; it shall be secured with tamperproof screws. A wall mount and a ceiling/pole mount shall be available. The camera dome shall have an IP66 and IK10 rating. The camera shall provide a Micro SD card slot for local storage.

K.	An event map shall be available to establish a schedule for each event trigger from the camera; up to 15 events shall be able to be registered.

L.	16 individual programmable privacy masks shall be available to hide certain areas for display on screen.

M.	Motion detection capability shall be available. There shall be 16 configurable zones for motion detection. Each zone shall be individually configurable for threshold, sensitivity and dwell time levels. 

N.	The capability to flip (invert) the video image shall be available. This feature is useful when mounting units in an inverted position.

O.	The dome shall have a maximum video transmission rate of 60 fps (50 fps PAL) dual stream or 30 fps (25 fps PAL) triple stream.

P.	Two-way audio shall be provided.

Q.	The dome shall be capable of 10 simultaneous viewing/recording streams per camera.

2.03	NETWORK VIDEO TRANSMISSION

A.	Compression:		H.265/H.264, M-JPEG
B.	Video Output:		3 MP @ 30 fps
C.	Protocols:		IPv4/IPv6, HTTP, HTTPS, RTSP/RTP, RTCP, QoS, FTP, TCP/IP, DHCP, UDP, uPnP, DDNS, Zeroconfig, Bonjour, ONVIF

2.04	CAMERA SPECIFICATIONS

D.	Imaging Device:		1/2.8-inch progressive scan CMOS
E.	Maximum Resolution:	3 MP (2048x1536) 
F.	Shutter Speed:		1 to 1/10,000 sec
G.	Gain Control:		Automatic/Manual
H.	WDR	:	On/Off selectable; 120 dB
I.	Backlight Compensation:	On/Off selectable 
J.	Sensitivity:	Color: 0.35 lux 
B&W: 0.013 lux, IR LED On @50 IRE; 0 lux, IR LED On.
K.	Iris Control:		Automatic/Manual
L.	Video Focus:		Automatic/Manual
M.	White Balance:		Automatic/Manual; red/blue gain adjustable
N.	Lens:		4.6 – 165 mm (36X optical zoom), f/1.6; 
                    1.9° – 58.1° horizontal angle of view 

2.05	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	12 VDC; uPoE (injector included)
B.	Current (IR On):	2.3 A @ 12 VDC; 500 mA @ PoE
C.	Power Consumption:	28 W 
D.	Power Connector:	12 VDC jack 
E.	Network/PoE Connector:	RJ-45 CAT 5
F.	Audio Connector:	Jack; audio out requires external amplifier
G.	Alarm Input/Output:	Screw terminal block (4 alarm in/1 alarm out)
H.	Video Out:	RJ-45 connector
I.	Radio Frequency	
	Emission Rating: 	FCC Class A

2.06	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-22° to 149°F (-30° to 65°C)

2.07	PHYSICAL SPECIFICATIONS

A.	Dimensions		Diameter: 7.9-in. (201 mm).
Height: 12.5-in. (317.8 mm).
		
B.	Weight: 			11.2 lb (5.1 kg)

2.08	MECHANICAL SPECIFICATIONS

A.	Application:	Outdoor; IP66; IK10

2.09	CERTIFICATIONS

A.	FCC, Class A
B.	CE
C.	ONVIF
D.	IP66
E.	IK10

2.10	WARRANTY

A.	3 years, parts and labor 

2.11	APPROVED MANUFACTURERS

A.	The camera dome shall be Vicon Industries Model SN683D-WIR. The wall mount shall be model V670-HDB242; the pole/ceiling mount shall be model V670-HDB241.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.
Surveyor is a trademark of Vicon Industries Inc. in the United States and other countries.