Vicon® Industries V2100D OUTDOOR IP DOME CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP DOME CAMERA 

A.	The outdoor dome camera shall incorporate a fixed camera/lens combination. The dome camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera be available in 2 MP and 5 MP resolution models and shall have true WDR and Smart IR capability and include an integral varifocal DC-iris lens; both the 2MP and 5 MP models shall have a 3.1-10 mm lens. The lens shall be available motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 98 ft (30 m) with 16 IR LEDs. 

B.	The camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and rotation (roll), for any angle of view required. A variety of mounting options shall be available. 

C.	The dome camera shall be powered by PoE or 12 VDC. 

D.	The dome camera shall have triple streaming video and support H.264/H.265 and 
M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity.

E.	Camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection. It shall have Video Content Analysis (VCA) of motion and tampering/defocus.

F.	The dome camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/Q interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

G.	The dome camera shall provide a slot for an SD card for local storage.

H.	The dome camera shall meet or exceed the following design and performance specifications.

2.03	DAY/NIGHT IP DOME CAMERA SPECIFICATIONS

A.	Imaging Device:	1/2.8-inch progressive scan 
B.	Max. Resolution:	2 MP and 5 MP models
C.	Shutter Speed:	1/2 - 1/10,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity(@30 IRE):	2 MP: Color: 0.015 lux; B&W: 0.005 lux/0 lux (IR Off/On)
5 MP: Color: 0.05 lux; B&W: 0.03 lux/0 lux (IR Off/On)
F.	Tilt and Horizontal	Two-direction adjustment, allowing for adjustment of 
                                              pan and tilt
G.	Digital Zoom:	Yes (ROI)
H.	Lens Adjustment:	Motorized lens, DC-iris 
I.	Focal Length:	3.1-10 mm varifocal 
J.	Horizontal Field of View:	2 MP: 102°-34° (wide-tele); 5 MP: 96°-32° (wide-tele)
K.	Vertical Field of View:	2 MP: 54°-20° (wide-tele); 5 MP: 69°-24° (wide-tele)
L.	Depth Field of View:	2 MP: 118°-40° (wide-tele); 5 MP: 124°-40° (wide-tele)
M.	IR Distance:	Smart IR; 98 ft (30 m) with 16 IR LEDs

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	12 VDC or PoE
B.	Current:	PoE: 0.16 A; 12 VDC: 0.63 A 
C.	Power Consumption:	IR On: 7.6 W;  IR Off: 5.2 W
D.	Connectors:	Pigtail cable provided; optional backbox required for
                                             cabling
                                             Power: 12 VDC terminal block
	PoE: RJ-45
		Video/Data: RJ-45
		Slot for SD card (128 G max customer supplied card)
		Reset button
		Default button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-22° to 140°F (-30° to 60°C)
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum alloy body; bracket: PC+ABS; 
                                             window: double glass/polycarbonate
B.	Dimensions:	Diameter: 5.3 in. (135 mm), 
Height: 4.4 in. (112 mm)
C.	Weight: 	2.2 lb (1 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	3-axis camera adjustment: pan >355°; tilt 0°-80°,
rotate ±355°

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	2 MP: 1920x1080, 1280x960/720, 800x600, 640x480, 
5 MP: 2592x1944/1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480
Max 30 fps 
F.	Web Browser:	Internet Explorer, Safari, Firefox, Chrome, Microsoft 
                                             Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             motorized zoom and focus (lens); dynamic ROI
I.	Video Content Analysis 
(VCA):	Tampering/defocus, motion
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/Q/T

2.09	CERTIFICATIONS

A.	CE
B.	UL
C.	FCC, Class A
D.	IP67
E.	IK10
F.	ONVIF S/T/G/Q
G.	RoHS
H.	NDAA/GSA/TSA compliant

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP bullet camera shall be Vicon Industries V2102D-W313MIR and V2105D-W313MIR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.