Vicon® Industries PS-24P INTELLIGENT NETWORK SWITCH
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	INTELLIGENT NETWORK SWITCH

A.	The switch shall have 24 PoE+ ports and a total 380 W PoE budget. The network shall be able to be tailored to service clients according to their particular speed requirements and shall be perfect when large files must be moved across the network quickly. The unit shall use RJ-45 type connectors for network connection. Two SFP ports to allow fiber connection shall also be provided. PoE technology shall automatically balance the load required for each device. 

B.	The switch shall be able to integrate with a system running PoE. Power control circuitry shall automatically detect Power over Ethernet (PoE) on access devices before providing power.

C.	An intuitive web GUI shall allow simple web management. This smart switch shall support Layer 2 switching basic features as well as some advanced Layer 3. It shall support HTTP and HTTPS, providing a secure graphical interface. It shall support full duplex.

D.	LED indicators shall provide power status and port speed/link/activity per port.

E.	The network switch shall comply with FCC limits for a Class A computing device in accordance with the specifications in Part 15 of FCC.

F.	The switch shall allow rack mount installation.

G.	The switch shall have the following mechanical specifications:

2.03	NETWORK SPECIFICATIONS
	A. CPU:			500 MHZ MIPS-4KEc; 128 MB RAM; 32 MB SPI Flash
	B. Packet Buffer Memory:	512 KB (dynamically shared across used ports only)
	C. Forwarding Modes:		Store-and-forward
	D. Bandwidth:			52 Gbps (non-blocking, full duplex)
	E. Multicast Groups:		128
	F. Number of VLANS:		64

2.04 	ELECTRICAL SPECIFICATIONS
A.	Input Power: 		Internal power supply
B.	Power Consumption:	32.71 W max power (all ports used, line-
					rate traffic); 446.7 W max power (all ports used, full PoE,
                                                    line-rate traffic)
Total PoE Budget:		380 W (30 W per port)

2.05	PHYSICAL SPECIFICATIONS

A.	Dimensions:		Height: 1.7 in. (43 mm) 
		Width: 17.3 in. (440 mm)
		Depth: 8.0 in. (204 mm)
	
B.	Weight: 	8.18 lb (3.7 kg)

2.06	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	32° to 122°F (0° to 50°C)

2.07	CERTIFICATIONS

A.	CE
B.	FCC, Class A
C.	UL
D.	CSA

2.08	WARRANTY

A.	3 years, parts and labor 

2.09	APPROVED MANUFACTURERS

A.	The switch shall be Vicon Industries Model PS-10PP-240 and PS-10PP-480.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.