Vicon® Industries V2000B OUTDOOR IP BULLET CAMERA 
	SECURITY SYSTEM
28 23 00 VIDEO SURVEILLANCE

PART 2 - PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.

2.02	OUTDOOR IP BULLET CAMERA 

A.	The outdoor bullet camera shall incorporate a fixed camera/lens combination. The bullet camera shall be available for indoor/outdoor surface mounting. The high-resolution day/night camera be available in 2 MP, 5 MP and 8 MP resolution models and shall have true WDR and Smart IR/Adaptive IR capability and include an integral varifocal DC-iris lens; the 2/5 MP models shall have a 3.1-10 mm lens and the 8 MP shall have a 3.6-10 mm lens. The lens shall be available motorized to allow for remote configuration of zoom and focus (motorized focus and zoom). Day/night operation shall be achieved using a built-in IR-cut filter. IR distance shall be 131 ft 
(40 m) with 4 IR LEDs. 

B.	The camera position shall have a three-direction adjustment, allowing for adjustment of pan, tilt and rotation (roll), for any angle of view required. A variety of mounting options shall be available. 

C.	The camera shall provide Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line counting/cross, loitering, object left/removed, wrong direction and area counting. 

D.	The bullet camera shall be powered by PoE, 24 VAC or 12 VDC. A dual heater system shall be provided that maintains proper temperature in the camera housing and prevents fogging of the window.

E.	The bullet camera shall have triple streaming video and support H.264/H.265 and 
M-JPEG compression. The camera shall also have smart encoding to further improve video encoding and improve storage capacity.

F.	Camera features shall include electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.

G.	The bullet camera shall meet the FCC requirements for a Class A device. It shall include support for the industry-standard ONVIF S/T/G/Q interface. It shall be IP67-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance, including front glass. The camera shall meet the latest regulations required to be NDAA, GSA schedule and TAA approved.

H.	The bullet camera shall provide a slot for an SD card for local storage.

I.	The bullet camera shall meet or exceed the following design and performance specifications.
2.03	DAY/NIGHT IP BULLET CAMERA SPECIFICATIONS

A.	Imaging Device:	2/5MP: 1/2.8-inch progressive scan 
                                             8 MP: 1/1.8-inch progressive scan
B.	Max. Resolution:	2 MP, 5 MP and 8 MP models
C.	Shutter Speed:	1/2 - 1/10,000 sec
D.	Automatic Gain Control:	On/Off selectable
E.	Sensitivity (@30 IRE):	2 MP: Color: 0.007 lux; 
B&W: 0.002 lux/0 lux (IR Off/On)
5 MP: Color: 0.03 lux; B&W: 0.01 lux/0 lux (IR Off/On)
8 MP Color: 0.02 lux; B&W: 0.01 lux/0 lux (IR Off/On)
F.	Tilt and Horizontal	Three-direction adjustment, allowing for adjustment of 
                                              pan, tilt and rotation (roll)
G.	Digital Zoom:	Yes (ROI)
H.	Lens Adjustment:	Motorized lens, P-iris automatically adjusts to zoom 
                                              condition
I.	Focal Length:	2/5 MP: 3.1-10 mm varifocal 
                                             8 MP: 3.6-10 mm varifocal
J.	Horizontal Field of View:	2 MP: 110°-34° (wide-tele); 5MP: 96°-32° (wide-tele);
                                             8 MP: 98°-46° (wide-tele)
K.	Vertical Field of View:	2 MP: 58°-20° (wide-tele); 5 MP: 69°-24° (wide-tele);
                                             8 MP: 54°-26° (wide-tele)
L.	Depth Field of View	2 MP: 134°-40° (wide-tele); 5MP: 124°-40° (wide-tele);
                                             8 MP: 113°-54° (wide-tele)
M.	IR Distance:	Smart IR/Adaptive IR; 131 ft (40 m) with 4 IR LEDs
N.	Dual Heater System:	For low temperature operation: heater turns on at -40° F 
                                             (-40° C) and off at 59° F (15° C). 
                                             For defog operation: heater turns on at -40° F and off at
                                             140° F (60° C).

2.04	ELECTRICAL SPECIFICATIONS

A.	Input Voltage:	24 VAC (+20%/-10%), 12 VDC (±10%) or PoE+
B.	Current:	2 MP: PoE: 0.39 A; 24 VAC: 0.78 A; 12 VDC: 1.56 A 
                                             5 MP: PoE: 0.42 A; 24 VAC: 0.83 A; 12 VDC: 1.67 A
                                             8 MP: PoE: 0.41 A; 24 VAC: 0.82 A; 12 VDC: 1.64 A 
C.	Power Consumption:	IR/Heaters On: 2 MP: 18.72 W; IR Off/Heaters On: 11.52 W
                                             IR/Heaters On: 5 MP: 20 W; IR Off/Heaters On: 14 W
                                             IR/Heaters On: 8 MP: 19.68 W; IR Off/Heaters On: 12.48 W
D.	Connectors:	Pigtail cable provided; optional backbox required for
                                             cabling
                                             Power: 12 VDC or 24 VAC terminal block
	PoE: RJ-45
		Video/Data: RJ-45
		Alarm: screw terminal
		Audio: screw terminal; audio level alarm alert
		Slot for SD card (128 G max customer supplied card)
		Reset button
		Default button
E.	Radio Frequency	
	Emission Rating: 	FCC Class A; CE

2.05	ENVIRONMENTAL SPECIFICATIONS

A.	Operating Temperature:	-40° to 140°F (-40° to 60°C)
	
B.	Humidity:	Up to 90% relative, non-condensing

2.06	PHYSICAL SPECIFICATIONS

A.	Construction:	Aluminum alloy body; sunshield: PC+ABS
B.	Dimensions:	Length: 10.3 in. (261 mm), 
Diameter: 3.5 in. (89 mm)
C.	Weight: 	4 lb (1.8 kg)

2.07	MECHANICAL SPECIFICATIONS

A.	Camera Mount:	Surface mount 
B.	Adjustments:	3-axis camera adjustment: pan 360°; tilt 0°-90°; 
roll 360° 

2.08	NETWORK VIDEO SPECIFICATIONS

A.	Communication Platform:	Open platform; compatible with Valerus 
	Video Management System 
B.	Compression:	Smart Encoding; H.264/H.265; M-JPEG 
C.	LAN Interface:	10 Base-T/100 Base-TX, Unicast/Multicast
D.	Video Channels	Triple streaming
E.	Resolution and Frame Rate:	2 MP: 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240 
5 MP: 2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180
8 MP: 3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240
Max 30 fps 
F.	Web Browser:	Internet Explorer, Safari, Firefox, Chrome, Microsoft 
                                             Edge
G.	Users:	Live viewing for up to 10 clients
H.	Image Settings:	Digital image effects defog, flip and mirror; configurable 
                                             brightness, contrast, saturation, hue, sharpness; BLC; 
                                             HLC; gamma correction; 3 DNR; motion detection; 
	white balance, AGC; Electronic Shutter, automatic or 
	manual; digital zoom; motion detection; privacy masks;
                                             motorized zoom and focus (lens); dynamic ROI
I.	Intelligent Video Analytics:	Tampering/Defocus, Intelligent Motion Detection 
                                             Intrusion Detection; Line Counting/Cross, Loitering, 
                                             Object Left/Removed, Wrong Direction, Area Counting
J.	Supported Protocols:	IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, 
                                             RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, 
                                             HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, 
                                             DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF 
                                             S/G/Q/T

2.09	CERTIFICATIONS

A.	CE
B.	UL
C.	FCC, Class A
D.	IP67
E.	IK10 (including front glass)
F.	ONVIF S/T/G/Q
G.	RoHS
H.	NDAA/GSA/TSA compliant

2.10	WARRANTY

A.	3 years, parts and labor

2.11	APPROVED MANUFACTURERS

A.	The outdoor IP bullet camera shall be Vicon Industries V2002B-W313MIR, V2005B-W313MIR and V2008B-W310MIR.

END OF SECTION

Vicon is a registered trademark of Vicon Industries Inc. in the United States and other countries.