PART  2  	PRODUCTS
2.1	GENERAL
A.	 All equipment and materials used shall be standard components, regularly manufactured, 
regularly utilized in the manufacturer’s system.
B.	All systems and components shall have been thoroughly tested and proven in actual use.
C.	All systems and components shall be provided with the availability of a toll free 24-hour 
immediate technical assistance for either the dealer/installer at no charge.
D.	All systems and components shall be provided with an explicit manufacturer warranty.
E.	All Cameras, NVRs, DVRs, and Workstations shall be available to be shipped pre-configured and programmed to the systems requirements by the manufacturer.
2.2	VIDEO MANAGEMENT SYSTEM
A.	Basis of Design:  Valerus Video Management System as manufactured by Vicon Industries.
** NOTE TO SPECIFIER ** Delete application server not required.
1.	Application Servers:  VLR-APPSRV-A (desk-top).
2.	Application Servers:  VLR-APPSRV-A-RK (rack-mount).
** NOTE TO SPECIFIER **  ‘X’ is the hard drive size. Delete recording servers not required.
3.	Recording Servers:  VLR-XTB-A (preloaded desk-top) 
4.	Recording Servers:  VLR-XTB-A-RK (preloaded rack-mount). 
5.	Recording Servers:  VLR-XTB-R5-A (internal RAID).
6.	Recording Servers:  VLR-MINI-XTBV1.
** NOTE TO SPECIFIER ** Delete viewing station not required.
7.	Viewing Stations:  VLR-CLIENT-A/VLR-CLIENT-4-A (desk-top; 2 or 4 monitor).
8.	Viewing Stations:  VLR-CLIENT-A-RK/VLR-CLIENT-4-A-RK (rack-mount; 2 or 4 monitor).
9.	Digital Video Recording Management and Network Software – General:
a.	Video Management Software (VMS):  Browser-based application meeting requirements of business and government surveillance applications.
1)	Web client with single point of management for entire system.
2)	Configuration Sections of Application:  Add, configure and operate recording servers, application servers, web servers, as well as IP cameras and encoders (edge devices).
3)	Operation and Maintenance Application:  Complete and comprehensive for video surveillance system.
4)	Full live digital video and audio surveillance over a standard 1 Gbps network.
b.	The VMS shall support recording, playback and archiving of video in standard industry compression formats, including H.265, H.264 and M-JPEG.
c.	True Open Standards (ONVIF) as Basis:  Thin client architecture. Centrally licensed. COTS compatible software or available preloaded on a manufacturer certified application/web server or recording server (NVR).
d.	Three License Tiers:  Associated with number of edge devices and a specific feature set. Licensing shall be based on a per edge device basis.
e.	COTS PCs with a minimum of Intel Core i7 processor, 16 GB of RAM and 5 GB of disk space for installation and a minimum of 75 GB of disk space for a recording device.
1)	Operating System:  Microsoft Windows 10 64-bit, 
2)	Operating System:  Microsoft Windows 2012, 2016 and 2019 64-bit Server.
3)	The Client (web) supports Windows 7 Operating systems.
f.	Software Features:  Easy to Use Tabs:  Access configuration screen and dashboard monitoring systems health. Monitoring Screen:  Video display area with available resources list. Multiple Display Views:  Configurable with variety layouts. Multiple Monitors:  Supported.
g.	Live Video:  Stream through Recording Server (NVR) with auto fail over to cameras. PTZ available from live video. Presets and tours are configurable. Digital zoom provided on video displays. 
h.	Web Based Interface:  
1)	Access the VMS from any standard web browser enabled device.
2)	Browser compatibility:  Internet Explorer 11 and Microsoft Edge. Chrome shall be able to be used with the Valerus Chrome extension from the Chrome store.
3)	Provide live viewing, playback and PTZ controls. 
4)	Mobile App:  Apple and Android smart phones and tablets. View live or recorded video. View concurrent multiple video streams; 4 on phones, 9 on tablets. Full control of PTZ, including presets. Quick and simple playback. Pinch to zoom on live and recorded video.
i.	Export Icon:  Easy access on display to save a video clip. Archived in MP4 format and authenticated in the player per the ONVF spec. 
j.	Playback:  Supported from main screen without leaving live video viewing area. Clicking Playback from time icon will allow selecting the playback to start from a specific date and time using standard calendar tools.
k.	Software Delivery:  Provided on manufacturer’s website.
l.	Events:  Setup in configuration area. Pre-Event Recording:  Supported and with event notification.
m.	Access Control System Support:  Accessed using a simple tab click. Interface opens in popup window that can be used in conjunction with the VMS. 
n.	Enhanced Edge-based Analytics:  Show bounding boxes around detected objects in live and playback video.
o.	Authorization roles shall be configurable; these roles shall then be listed in the Resources list on the monitoring display screen. This Resources list can be viewed in a hierarchy view with these groups or as a flat list.
p.	Video Masking:  Available centrally through the VMS. Allow users with the correct authority to unmask video as needed using icon on the display screen. Unmask feature available on live and playback video.
q.	Quick Configuration Wizard:  Streamlined process for typical and basic system setup with minimal input required.
r.	Search Functions:  Six search functions available including museum search, thumbnail search, events framework search, event search, audit log and Analytics Search.
s.	Capability for 360 degree lens dewarp available for use with cameras with fisheye lenses.
t.	Integration with Active Directory (AD):  Allow user management via the AD.
u.	Override mode:  Allows operating in case AD communication is lost.
v.	Multi-language Support:  All text in the user interface translated to selected language.
w.	Backup and Restore for system settings available.
x.	Keypads and PLC controls supported. Numeric IDs for devices configurable for use with controls. These devices shall be able to control remote monitors.
y.	Central Software Upgrade Interface:  Provides the ability to upgrade the entire system by pushing the upgrade from the Application Server to all devices on the system.
z.	System supports IPv4/IPv6 and HTTPS.
aa.	A Gateway module shall be available to bridge migration from a legacy ViconNet Video Management System to this VMS and use the old system resources.
bb.	The system shall have built in Log Collection from all system PCs, making it easier to troubleshoot problems. An advanced tool shall be provided.
cc.	The system shall accept external text strings from third party systems.
dd.	Alarm notification shall be both visual and audible.
ee.	A Report button shall generate an Excel report of the devices sorted by their hosting NVRs or a flat list.
ff.	Devices shall be able to be replaced or moved, for load balancing purposes.
gg.	An NVR Failover unit shall be able to be configured to take over in the event of an NVR failure.
hh.	A Mapping function shall be provided that allows the placement of resource devices on any imported map. The map shall be either a static or live map.
ii.	An Events Database shall exist to store any event that occurs in the system. From the Event Search screen, a query shall be able to be created to search for any event that occurs on the system from any resource in the system.
jj.	A video clip, either in live or playback, shall be able to be bookmarked for easy referral.
kk.	The ability to use mobile devices as mobile cameras shall be available. The mobile device shall be able to receive event alerts.
ll.	The VMS shall be able to accept partner systems through an integration framework.
mm.	A Snapshot function shall be provided to capture video from live or playback; this snapshot shall be able to be saved. It shall be possible to capture snapshots from all resources and update them all at the same time.
nn.	An Audit Log shall be available to track every user’s actions.
oo.	Keypads/PLC shall have the ability to call up other remote monitors. 
pp.	A thick-client solution shall be available for users who don’t want to use a browser.
qq.	Shall be operational in a virtual environment.
rr.	An integration framework shall be provided to allow partnerships with third party systems such as LPR and Access Control.
ss.	An Alarms Management module shall be provided that shall allow events to be defined as alarms and provide tools to review open alarms and close them. Alarms shall have a defined life cycle and procedures shall be able to be created to handle these alarms, if needed.
tt.	A Client Performance Indicator shall be provided to indicate system performance as more cameras are added and displayed.
uu.	The system shall have an enhanced dashboard that shall present the system’s health status and provide health monitoring information and statistics on all connected devices, including Application Server, NVRs and cameras. It shall provide notifications that notifications that provide cyber security and an easy-to-use activity mapping chart.
10.	Setup, Configuration and Security of VMS:
a.	Multi-User Authorization Login Application. 
1)	Offer levels of authorization based on functions. 
2)	Setup Utility:  Allows Administrator to configure additional users as well as user groups. 
3)	User authorization:  Configurable for specific system operations. Authorization Permission Setup:  Performed using the User screen. 
4)	Authorization Roles:  Available to configure from the Authorization Roles screen. Permissions:  Provide authority to perform all system functions. 
5)	Users and groups on AD servers may be imported and become a group in the VMS.
6)	The software shall offer a full multi-user authorization process as follows:  Authorization Roles:  Created once globally. Authorized and given specific permissions. Users:  Created once globally and may be given rights to groups. No virtual limit on number of groups and users authorized in the software. Authorization Roles to be authorized or denied access to:  Monitoring screen for video display. Configuration. Dashboard. Video and audio (media) export. Override masking.
b.	A user, given appropriate access, may remotely configure components connected to the network. An access list shall be able to be created to add those PCs that are allowed to connect to Valerus, adding another layer of security.
c.	Software permits viewing of live video from any edge device connected to any recording server on the network.
d.	Export Icon:  Simplifies process of exporting video and creating archives and saving video to media, such as:  USBs, CD, DVDs or solid-state drives. An embedded player shall be optional with each exported/archived video clip for playback on any machine if configured to do so.
e.	Event Rules:  Create rules triggered by an event occurrence. Define actions executed for a given event. Events are selectable. Rules are configurable after an event is selected.
f.	Event Association:  Multiple devices may be associated with an event. Actions Triggered by Event:  Configurable as On and Off. Display live video. Display a view. Go to a preset. Operate a relay. Run a PTZ tour. Run a view tour. Start a URL. Delay function.
g.	Scheduled Recordings:  Applies to cameras, encoders and microphones. Scheduling is based on rules configurable for actions the system takes upon an event. Schedules accessible on recording tab in device configuration. Create and Schedule Recordings:  By authorized users. How often schedules repeat; weekly, monthly, yearly or never. Determines how the systems prioritizes schedules if schedule times overlap. Schedules available when configuring recording and rules, saving the need to create multiple and duplicate schedules. Sequencing cameras, including multi-screen displays. Record cameras at different qualities and frame rates from any recorder on the network. Schedule shall allow running preconfigured combinations of camera, sensor and PTZ programmed routines.
h.	System Components:  Application/Web Server:  Act as main system server; Windows based. Global configuration of the system is stored on this server. Recording Servers (NVRs):  Windows based providing communication, live streaming, recording, video playback and audio from cameras and encoders.
i.	Device Configuration:  Valid devices to be configurable for system recognition and operation. Cameras, fixed or with integrated PTZ. Microphones. Encoders. Sensors. Relays.
j.	Authentication:  Video from cameras are enabled to verify the authentication of the video and present an authentication symbol on the displayed video for recorded playback through the player when enabled only on export.
11.	User Interface for VMS:
a.	User Friendly Tabs:  Allow monitoring of live and playback video, and configuration of the system.
b.	Login Window:  Consists of User Name and Password fields. Default User Name and Password:  Available for initial login. Configurable for increased security; there shall be an option to enforce a complex password.
c.	Serve operators, supervisors and system administrators. 
d.	Monitoring Display Screen:  
1)	Selection of number of tiles to display. 
2)	Resource list of devices in system. Viewable as flat list or hierarchical list based on user configured groups. Resources include names of devices and icons depicting devices. Video Channels (cameras) connected, differentiating between PTZ and fixed cameras. Audio Channels (microphones). Views. Tours. Web Pages. Relay Outputs.
3)	Display Area:  Offers display configurations up to 36 tiles. Full screen View:  Available. More views added by clicking the plus sign to create new view tabs while not losing the default view. Controls:  Change the layout. Stop all displays. Export. Synchronize playback. Control current selected tab.
4)	Camera Controls:  Display at top of a tile when mouse hovers and may be locked in place. Playback. PTZ control. Digital zoom. Unmask. Export. Configuration settings
5)	Playback controls:  Visible when cameras go to playback. Looping a video section. Slow mode. Play from time. Rewind, fast rewind, pause, forward, and fast forward. Back to live video and current time.
6)	Access to all available programming menus.
7)	Viewing live devices is performed by dragging a device to any tile. Audio devices display in a smaller area below the video tiles.
e.	Dashboard, Search, Alarms and Configuration Menu Access:  Clicking a tab at the top of the screen.
12.	Video Quality for VMS:  Support any resolution video, jpeg and H.264 compression.
13.	Add-Ins for VMS
a.	Access Control Systems:  Available for integration.
1)	Meet requirements of business and government access control systems.
2)	Monitor and control facility access as well as video detection, temperature and communications loss monitoring.
3)	Provide control and access to users on Local Area Networks (LAN), Wide Area Networks (WAN), wireless networks and the Internet.
4)	Video viewing playback and PTZ control from the VMS.
b.	A method to add partner systems shall be provided through an integration framework. It shall support Thermal Radar sensor.
14.	Digital Servers:  Preloaded with Valerus VMS.
a.	Certifications:  UL, CE, FCC Class A.
b.	Application and Recording (NVR) Servers:  PC computer fully equipped with the Digital VMS, with an external monitor, keyboard and mouse for operation.
1)	Mini recording server.
** NOTE TO SPECIFIER **  LTSB is standard. The full Windows 10 operating system is available upon request.
2)	Operating System:  Microsoft Windows 10 LTSB (64-bit); Windows Server 2012, 2016 and 2019. 
3)	Operating System:  Microsoft Windows 10 (64-bit).
4)	Minimum Requirements:  Intel Core i7 processor. Intel Core i3 processor for the mini recording server. Memory:  16 GB of RAM. USB ports. Monitor outputs.
** NOTE TO SPECIFIER **  The desktop and 1U rack-mount versions support up to a certain drive size. Larger drive capacity is available, but may require a larger tower or 2U chassis. Contact your sales representative.
c.	Server Housing:  Desktop or rack-mount case with all suitable connectors available on the back panel. 
** NOTE TO SPECIFIER **  Delete if not required.
1)	Rack-mounting bracket kit.
d.	Server Capacities:
** NOTE TO SPECIFIER **  Delete recording servers and capacities not required.
1)	Recording Server Storage Capacity:  internal 1 TB hard-drive.
2)	Recording Server Storage Capacity:  internal 2 TB hard-drive.
3)	Recording Server Storage Capacity:  internal 3 TB hard-drive.
4)	Recording Server Storage Capacity:  internal 4 TB hard-drive.
5)	Recording Server Storage Capacity:  internal 6 TB hard-drive.
6)	Recording Server Storage Capacity:  internal 8 TB hard-drive.
7)	Recording Server Storage Capacity:  internal 10 TB hard-drive.
8)	Recording Server Storage Capacity:  internal 12 TB hard-drive.
9)	Recording Server Storage Capacity:  internal 14 TB hard-drive.
10)	Recording Server Storage Capacity:  internal 16 TB hard-drive.
11)	Recording Server Storage Capacity:  internal 20 TB hard-drive.
** NOTE TO SPECIFIER **  Delete application server not required.
12)	Application Server:  Standalone unit with no storage capability.
13)	Application Server:  All-in-one unit included in the recording server.
** NOTE TO SPECIFIER **  Delete mini recording servers not required.
14)	Mini Recording Server Storage Capacity:  internal 1 TB hard-drive.
15)	Mini Recording Server Storage Capacity:  internal 2 TB hard-drive.
16)	Mini Recording Server Storage Capacity:  internal 3 TB hard-drive.
17)	Mini Recording Server Storage Capacity:  internal 4 TB hard-drive.
18)	Mini Recording Server Storage Capacity:  internal 6 TB hard-drive.
19)	Mini Recording Server Storage Capacity:  internal 8 TB hard-drive.
** NOTE TO SPECIFIER ** Coordinate with system description for application and programmed function. RAID 5; available in RAID 6 with slightly lower storage capacities:  Delete if not required.
20)	Internal Raid Storage Device:  4-bay, 11 TB storage capacity.
21)	Internal Raid Storage Device:  4-bay, 17 TB storage capacity.
22)	Internal Raid Storage Device:  4-bay, 22 TB storage capacity.
23)	Internal Raid Storage Device:  4-bay, 34 TB storage capacity.
24)	Internal Raid Storage Device:  8-bay, 53 TB storage capacity.
25)	Internal Raid Storage Device:  12-bay, 62 TB storage capacity.
26)	Internal Raid Storage Device:  12-bay, 83 TB storage capacity.
27)	Internal Raid Storage Device:  12-bay, 104 TB storage capacity.
28)	Internal Raid Storage Device:  12-bay, 125 TB storage capacity.
29)	Internal Raid Storage Device:  24-bay, 174 TB storage capacity.
30)	Internal Raid Storage Device:  24-bay, 218 TB storage capacity.
31)	Internal Raid Storage Device:  24-bay, 262 TB storage capacity.
e.	Client Viewing Station:  Available with 2 or  4 or monitor outputs.
f.	Electrical Parameters for Digital Servers:
1)	Certifications:  UL, CE, FCC Class A.
2)	Input Voltage:  105 to 240 VAC, plus or minus 10 percent at 50 to 60 Hz.
3)	Current:  0.66 A at 115 VAC; 0.33 A at 240 VAC.
4)	4-bay internal storage:  5 A at 115 VAC; 3 A at 240 VAC
5)	8-bay internal storage:  9.5 A at 115 VAC; 4.5 A at 240 VAC.
6)	12-bay internal storage:  10 A at 115 VAC; 8 A at 240 VAC
7)	24-bay internal storage:  10 A at 115 VAC; 8 A at 240 VAC.
8)	Power Consumption:  76 W; mini:  38 W. 4-bay internal storage:  300 W, includes redundant power supply. 8-bay internal storage:  650 W includes redundant power supply. 12-bay internal storage:  875 W includes redundant power supply. 24-bay internal storage:  975 W; includes redundant power supply.
9)	CPU:  Intel Core i7. Mini:  Intel i3.
10)	RAM Memory:  16 GB minimum.
11)	Heat Output:  266 btu/hour. Mini:  133 btu/hour.
12)	Storage:  1 TB to 20 TB. Depending on model.
13)	Operating System:  Microsoft Windows 10 LTSB.
14)	Operating System:  Microsoft Windows 10.
15)	LAN Interface:  100/1000 Base T Ethernet interface on main board.
16)	Front Panel Controls and Indicators:  Power, network activity LEDs, USBs.
15.	Mechanical Parameters.
a.	Application:  Indoor.
b.	Mounting:  Desktop, mini desktop or rack unit mounted in a standard EIA compliant rack, 19 in. (483 mm) wide opening. Rack height is 1.75 in. (44 mm) or 1 RU.
c.	Rack Weight:  18.2 lbs (8.3 kg) approximately.
d.	Rack Dimensions:  Width (W):  19.0 in. (483 mm). Depth (D):  16 in. (406mm). Height (H):  1.75 in. (44.45 mm), 1 RU.
e.	Four-Bay Internal Storage Weight:  28.7 lbs (13 kg).
f.	Four-Bay Internal Storage Dimensions:  Width (W):  19 in. (483 mm). Depth (D):  22 in. (660 mm). Height (H):  1.75 in. (89 mm).
g.	Eight/Twelve-Bay Internal Storage Weight:  46.3 lbs (21 kg).
h.	Eight/Twelve-Bay Internal Storage Dimensions:  Width (W):  19 in. (483 mm). Depth (D):  26 in. (660 mm). Height (H):  3.5 in. (89 mm).
i.	Twenty-four-Bay Internal Storage Weight:  82.0 lbs (37 kg).
j.	Twenty-four-Bay Internal Storage Dimensions:  Width (W):  19 in. (483 mm). Depth (D):  27.5 in. (711 mm). Height (H):  6.9 in. (176 mm).
k.	Desktop Weight:  8.1 lbs (3.7 kg) approximately. Mini:  2.5 lbs (1.1 kg).
l.	Desktop Dimensions:  Width (W):  3.75 in. (95.25 mm). Depth (D):  10.5 in. (266.7 mm). Height (H):  9.5 in. (241.3 mm). Mini:  Width (W):  7.9 in. (200 mm). Depth (D):  7.75 in. (197 mm). Height (H):  3.5 in. (89 mm).
m.	Construction:  Steel and plastic.
n.	Color:  Black.
16.	Environmental Parameters:
a.	Operating Temperature Range:  32 to 104 degrees F (0 to 40 degrees C).
b.	Operating Humidity Range:  0 to 95 percent, non-condensing.
** NOTE TO SPECIFIER ** Delete encoder subparagraph if not required or delete basis of design subparagraph not required.
17.	Encoders:
a.	Basis or Design:  VLR-ENC-16 Sixteen Channel ONVIF Video Encoder as manufactured by Vicon Industries.
1)	Ideal solution for creating hybrid analog/IP systems using analog cameras with IP VMS.
2)	Supports AHD, TVI and analog cameras up to 960H resolution.
3)	Video Input:  Sixteen analog camera video input.
4)	Video Output:  CVBS, VGA and HD.
5)	Compression:  H.264.
6)	Streaming:  Dual.
7)	Auto-sensing:  NTSC/PAL.
8)	Transmission Rate:  Up to 480 fps at D1/960H/720P resolutions; 240 fps at 1080P resolution.
9)	Alarms:  Four inputs, one relay control output.
10)	PTZ port and four RCA audio inputs and one RCA audio output.
11)	Privacy masking and motion detection.
12)	Input voltage:  12 VDC; dual voltage (110/220 VAC) power supply provided.
13)	ONVIF Interface:  Interoperability open platform systems.
b.	Manufacturer requires the use of uninterruptible power supply systems (UPS) to prevent voltage fluctuations that can affect operation and cause damage to the equipment. Failure to comply voids the warranty.
** NOTE TO SPECIFIER **  Delete paragraph if not required
** NOTE TO SPECIFIER ** Delete if not required.
2.3	VIRTUAL MATRIX DISPLAY CONTROLLER
A.	Virtual Matrix Display Controller (VMDC) as manufactured and supplied by Vicon Industries.
1.	Certifications:  FCC Class A.
2.	Models:
** NOTE TO SPECIFIER ** Component options. Coordinate with system description for application and programmed function. The Virtual Matrix Display Controllers specified are compatible with either the Valerus or ViconNet Video Management systems. Delete models not required.
a.	VMDC-SW:  Virtual Matrix Display Controller Software (Installation on 3rd party server). Single license. 
b.	VMDC-2:  Virtual Matrix Display Controller with 2 display outputs. Tower unit.
c.	VMDC-4:  Virtual Matrix Display Controller with 4 display outputs. Tower unit.
d.	VMDC-6:  Virtual Matrix Display Controller with 6 display outputs. Tower unit. 
e.	VMDC-2R:  Virtual Matrix Display Controller with 2 display outputs. 4RU rack-mount unit.
f.	VMDC-4R:  Virtual Matrix Display Controller with 4 display outputs. 4RU rack-mount unit.
g.	VMDC-6R:  Virtual Matrix Display Controller with 6 display outputs. 4RU rack-mount unit.
h.	The viewer application shall be Vicon's VN-VIEWER-16.
3.	Self-contained, matrix control solution for the VMS. Direct network video to multiple monitor displays using a keypad, graphical user interface (GUI) or Programmable Logic Controller (PLC). 
a.	Events Management system in the VMS software receives data from external systems, triggering macros in response to the input. 
b.	Matrix command/control center software interface and hardware decoding component enable remote network video streams to be displayed on multiple monitors in multiple locations. Operator can display any camera on any monitor connected to the network. Camera selection may be controlled via a dedicated keypad or by using the graphical user interface. 
c.	Scalable. A single VMDC unit controls up to 6 high-definition monitors. Control additional monitors by connecting additional VMDC units to the network and/or using video decoder appliances.
d.	Enclosures:  Rack or tower. 
e.	Software available for installation on a PC meeting minimum requirements specified in this document.
4.	Software Description:  Graphic user interface (GUI) incorporating video display areas, toolbars, control palettes, and site/device lists. The system allows camera-to-monitor selection and camera PTZ control on a keypad controller or PLC.
a.	Receives live or recorded video inputs. Operators can direct the video to any monitor connected to it, including monitor walls or monitors connected to additional VMDCs on the network. Available licensing for 2, 4 or 6 monitors. Licenses upgradeable at any time to maximum of 6 monitors. 
b.	Each VMDC supports 4 keypads/serial host interface. 

** NOTE TO SPECIFIER **  Component options. Coordinate with system description for application and programmed function. The cameras listed below are compatible with either the Valerus or ViconNet Video Management System. Delete the cameras not required.
2.4	CAMERAS FOR VIDEO MANAGEMENT SYSTEMS
A.	General:
1.	All equipment and materials used shall be standard components, regularly manufactured, regularly utilized in the manufacturer’s system.
2.	All systems and components shall have been thoroughly tested and proven in actual use.
3.	All systems and components shall be provided with the availability of a toll free 24-hour immediate technical assistance for either the dealer/installer at no charge.
** NOTE TO SPECIFIER **  Delete PTZ cameras paragraph if not required.
B.	Pan-Tilt-Zoom (PTZ) Cameras:
** NOTE TO SPECIFIER **  Delete basis of design subparagraphs not required.
1.	Basis of Design:  V2002D-PTZ, Outdoor IP PTZ Network Compact Dome Camera as manufactured and Supplied by Vicon Industries.
a.	Certifications:  CE, UL, FCC, Class A, IP67, IK07, ONVIF S/T/G/Q, RoHS and NDAA/GSA/TSA compliant.
b.	General Features:
1)	Equipment and Materials:  Standard components regularly manufactured and used in manufacturer’s system.
2)	Systems and Components:  Tested and proven in actual use.
3)	Technical Support:  Toll free 24-hour phone number from manufacturer. No charge service for dealers and installers.
4)	Camera, lens, and pan/tilt drive in covert dome enclosure.
a)	Resolution:  2 MP with true WDR.
b)	Lens:  Integral varifocal 4.5-135 mm; 30X optical zoom.
c)	Day/night Operation:  Built-in IR-cut filter.
d)	Starlight low-light imaging.
e)	IR Distance:492 ft (150 m).
f)	Automatic Smart IR/Adaptive IR capability.
5)	Intelligent Video Analysis, tampering/defocus, intelligent motion detection, intrusion detection, line cross/counting, loitering, object left/removed, wrong direction and area counting.
6)	Powered By:  PoE, 24 VAC, or 48 VDC.
7)	Heater/Blower System:  Maintains proper temperature in camera housing and prevents window fogging.
8)	Triple Streaming Video and Network Video Transmission:  using either H.264/H.265 and M-JPEG compression.
a)	Smart Encoding:  Further improves video encoding and improves storage capacity.
b)	Transmits high quality video across network for remote viewing and recording.
c)	Configurable remotely from network digital video recorders and master workstations.
9)	Two Alarm Inputs:  Programmable for functional state (enabled or disabled); set to Normally Open (NO) or Normally Closed (NC).
10)	Alarm Outputs:  Control external equipment and may be set for Normally Open (NO) or Normally Closed (NC).
11)	An audio alert is available.
12)	Individual Programmable Preset Positions:  128. Each able to be titled and adjustable for pan and tilt speed and manual or auto focus.
13)	Four Tours (Patrols):  Available with 128 presets per tour. Each tour able to be titled and adjustable for pan, tilt, zoom speed, and dwell time. Programmed to repeat.
14)	Pan and Tilt Functions:  Programmable.
a)	Maximum Manual Pan and Tilt Speeds:  Programmable.
b)	Maximum Pan Speed:  300 degrees per sec.
c)	Maximum Tilt Speed:  160 degrees per sec.
d)	Pan and Tilt Speeds:  Scalable to zoom setting.
e)	Pan Range:  360 degree continuous.
f)	Tilt Range:  195 degrees (minus15 to 90 degrees).
15)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
16)	Meets FCC requirements for Class A device.
a)	Supports industry-standard ONVIF S/T/G/Q interface.
b)	IP67-rated to withstand rain, dust, and vandalism.
c)	IK7 rated for impact resistance.
d)	Meets latest regulations required to be NDAA, GSA schedule and TAA approved.
17)	Provide a slot for an SD card for local storage.
c.	Day/Night IP Dome Camera Specifications:
1)	Imaging Device:  1/2.8 inch progressive scan.
2)	Maximum Resolution:  2 MP.
3)	Shutter Speed:  1/30 to 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	WDR:  True WDR (120 dB).
6)	Sensitivity (at 30 IRE):  Starlight; Color:  0.007 lux; B and W: 0.002 lux.
7)	Pan/Tilt Range:  360 degree continuous pan; 95 degree tilt (minus 15 to 90 degree).
8)	Lens:  4.5 to 135 mm, 30X optical zoom.
9)	Digital Zoom:  10X.
10)	Lens Adjustment:  Motorized lens, P-iris automatically adjusts to zoom condition (manual mode).
11)	Horizontal Field of View:  60 minus 5 degrees (wide-tele).
12)	Vertical Field of View:  38-3 degrees (wide-tele).
13)	IR Distance:  492 ft (150 m); Smart IR/Adaptive IR automatic IR 
14)	Heater/Blower System:  For low temperature operation. Heater turns on at 59 degrees F (15 degrees C); blower is always on.
d.	Electrical Specifications:
1)	Input Voltage:  24 VAC, 48 VDC or PoE.
2)	Current:  24 VAC:  2.5 A; 48 VDC:  1.25 A.
3)	Power Consumption:  Total 36.4 W.  PTZ 11 W; IR:  19 W; Heater:  5,5 W; Blower:  0.9 W.
4)	Connectors:  Power: 48 VDC or 24 VAC terminal block; PoE:  RJ-45.
a)	Video/Data:  RJ-45.
b)	Alarm:  Screw terminal.
c)	Audio:  Screw terminal.
d)	Slot for SD card (128 G max customer supplied card).
e)	Reset button.
f)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
e.	Environmental Specifications:
1)	Operating Temperature:  Minus 40 to 140 degrees F (Minus 40 to 60 degrees C).
2)	Humidity:  Up to 90 percent relative, non-condensing.
f.	Physical Specifications:
1)	Construction:  Aluminum base; polycarbonate clear dome.
2)	Dimensions:  Height: 13.2 inches (336 mm).
3)	Diameter:  7.5 inches (190 mm).
4)	Weight:  11.5 lbs (5.2 kg).
g.	Mechanical Specifications:
1)	Camera Mount:  Mounting accessories available.
2)	Adjustments:  Pan 360 degrees continuous; tilt: 95 degrees (-15 degrees -90).
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution and Frame Rate:  1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240 Max 30 fps.
6)	Web Browser:  Internet Explorer, Safari, Firefox, Chrome, Microsoft Edge.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
9)	Intelligent Video Analytics:  Tampering/Defocus, Intelligent Motion Detection Intrusion Detection; Line Counter/Cross, Object Left/Removed, Wrong Direction, Area Counting.
10)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF, S/G/Q/T.
2.	Warranty:  3 years, parts, and labor.Basis of Design:  SN673V-C Cruiser Network Dome Cameras as manufactured and supplied by Vicon Industries:
a.	Certifications:  CE, FCC Class A, ONVIF Profile S Compliant.
b.	General Features:
1)	Mounting:  Surface mountable. Wall, corner and pole mounting accessories available.
2)	Camera/Lens:  1/1.7-in. progressive scan CMOS day/night with a 4.7-94 mm varifocal lens (optical 20x; 16X digital zoom). 
3)	Outdoor model:  IP66 rating with pan/tilt drive. Covert enclosure. 
4)	Dome:  Clear polycarbonate secured by tamperproof screws.
5)	Quad-streaming network video transmission using open platform H.264/H.265 or M-JPEG compression (3x H.264/H.265 and 1x M-JPEG) for remote viewing and recording. ONVIF interface enabling third party software recording.
6)	Configurable remotely from network digital video recorders and master workstations
7)	Alarm Inputs:  Four, individually programmable NO or NC. 
8)	Alarm output. One.
9)	Programmable Preset Positions:  256.
10)	Tours:  8 tours. 
11)	Configuration:  High level, programmable functions via a web browser. Gain control:  Adjustable. White balance gain using red and blue scales. Shutter speed:  Automatic or manual. Backlight compensation or Wide Dynamic Range:  Programmable. Digital Noise Reduction:  Programmable on or off.
12)	Real time clock and scheduler:  Programmable for each day of the week. 15 programmable events. A schedule can be established for each event trigger.
13)	Privacy Masks:  16 programmable.
14)	Motion Detection:  16 windows for motion detection (8 include, 8 exclude). Sensitivity level programmable for each window. 
15)	Image Inverting:  
16)	Multilanguage menu system.
17)	Video Transmission Rate:  30 fps.
18)	Audio input:  1 audio in. 1 audio out.
19)	Viewing Streams:  10 live simultaneous and 3 playbacks per camera.
20)	Micro SD card slot for local storage.
c.	Camera Parameters:
1)	Imaging Device:  1/1.7-inch progressive scan CMOS
2)	Resolution:  2 MP (1080p) resolution.
3)	Shutter Speed:  1/3 to 1/30,000 sec.
4)	Gain Control:  Automatic and Manual
5)	Wide Dynamic Range (WDR):  120 dB; WDR on/Off selectable.
6)	Backlight Compensation:  On/Off selectable.
7)	Sensitivity:  Color:  0.35 lux. Black and White:  0.13ux, at 50IRE.
8)	Adjustment, Pan and Tilt:  Continuous Pan:  360 degrees. Tilt:  180 degrees with digital flip. Pan speed:  380 degrees/sec. Tilt speed:  380 degrees/sec on preset. Variable speed:  0.1 to 380 degrees per sec. 
9)	Iris Control:  Automatic/Manual.
10)	Video Focus:  Automatic/Manual (near-far).
11)	White Balance:  Automatic/Manual; red/blue gain adjustable.
12)	Digital Noise Reduction:  Programmable On/Off.
13)	Lens:  4.7 to 94 mm; 55.5 to 3 degrees horizontal angle of view
d.	Electrical Parameters:  
1)	Input Voltage:  PoE; 24 VAC; 12 VDC. Maximum 12 W power consumption.
2)	Connectors, Power:  2-position removable screw terminal block.
3)	Connectors, Alarm Input:  8-position removable screw terminal block.
4)	Connectors, Network:  RJ-45 CAT 5.
5)	Connectors, Audio:  Two 1/8 in (3 mm) phono jacks.
6)	Connectors, Video Out:  RJ-45.
7)	Connectors, Relay:  4-position removable screw terminal block.
8)	Radio Frequency Emission Rating:  FCC Class A.
e.	Physical Parameters:
1)	Operating Temperature:  Minus 14 to 122 degrees F (minus 10 to 50 degrees C) in accordance with NEMA 2.1.5.1 STD2.
2)	Dimensions (H x Diameter):  5.9 in (150 mm) x 6.1 in (154 mm).
3)	Dome:  4.3 in (110 mm) diameter.
4)	Weight:  3.5 lbs (1.6 kg).
f.	Network Parameters:  
1)	Compression:  H.265, H.264, M-JPEG.
2)	Video Output:  1920 x 1080 at 30 fps
3)	Programming Interface:  ONVIF Profile S, NTCIP.
4)	Protocols:  IPv4/IPv6, HTTP, HTTPS, RTSP/RTP, RTCP, FTP, uPnP, TCP/IP, DHCP, UDP, ARP, QoS, Zeroconfig, and Bonjour.
3.	Basis of Design:  SN693V Cruiser Network Dome Cameras as manufactured and supplied by Vicon Industries:
a.	Certifications:  
1)	FCC, Class A
2)	CE
3)	ONVIF Profile S compliant
4)	IP66
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24-hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Network Outdoor Camera Dome Features:
1)	Mounting:  Surface mountable. Wall, corner and pole mounting accessories available.
2)	Comprised of a high-resolution camera/lens and pan/tilt drive in an attractive covert enclosure.
3)	Camera/Lens:  1/2.8-inch progressive scan CMOS day/night with a 5-117 mm varifocal lens (optical 23x zoom). True wide dynamic range to provide the highest quality image with excellent and electronic image stabilization.
4)	Outdoor model:  Available with 1080p (2 MP) resolutions.
5)	Designed for easy installation.
6)	Lower Dome:  Constructed of impact-resistant polycarbonate. Secured by tamperproof screws. Several mounting options available.
7)	Triple-streaming network video transmission using open platform H.264/H.265 or M-JPEG compression (2x H.264 and 1x M-JPEG). ONVIF open architecture connectivity to enable third party software recording.
8)	Transmit high quality video across the network for remote viewing and recording and be configurable remotely from network digital video recorders and master workstations
9)	Alarm Inputs:  Four, individually programmable NO or NC. 
10)	Alarm output. One.
11)	Programmable Preset Positions:  256.
12)	Tours:  8 with 100 presets per tour. 
13)	Pan Range:  360 degree continuous and 90 degree tilt range with digital flip.
14)	Maximum Pan Speed:  380 degrees/sec. Maximum Tilt Speed:  380 degrees/sec on preset. Variable Speed:  0.1 degrees per sec to 38 degrees per sec. 
15)	Configuration:  High level, programmable functions via a web browser. Gain control:  Adjustable. White balance gain using red and blue scales. Shutter speed:  Automatic or manual. True Wide Dynamic Range:  Programmable. Digital Noise Reduction:  Programmable on or off.
16)	Real time clock and scheduler:  Programmable for each day of the week. 15 programmable events. A schedule can be established for each event trigger.
17)	Privacy Masks:  16 programmable. The masks shall be configurable to be solid or pixelated and a choice of colors shall be available.
18)	Motion Detection:  16 windows for motion detection (8 include, 8 exclude). Sensitivity level programmable for each window. 
19)	The capability to digitally flip (invert) the video image to be available. This feature is useful when mounting units in an inverted position.
20)	Multilanguage menu system.
21)	Video Transmission Rate:  30 fps.
22)	Audio input:  1 audio in. 1 audio out.
23)	Viewing Streams:  10 live simultaneous and 3 playbacks per camera.
24)	Micro SD card slot for local storage.
e.	Camera Parameters:
1)	Imaging Device:  1/2.8-inch progressive scan CMOS.
2)	Shutter Speed:  1 to 1/10,000 sec.
3)	Gain Control:  Automatic/Manual.
4)	Wide Dynamic Range (WDR):  120 dB; WDR On/Off selectable.
5)	Backlight Compensation:  On/Off selectable 
6)	Sensitivity:  Color:  0.35 lux; Black and White:  0.13ux, at 50IRE
7)	Iris Control:  Automatic/Manual.
8)	Video Focus:  Automatic/Manual (near-far).
9)	White Balance:  Automatic/Manual; red/blue gain adjustable.
10)	Digital Noise Reduction:  Programmable On/Off.
11)	Lens:  5 to 117 mm; 56.6 to 3 degrees horizontal angle of view.
f.	Electrical Parameters:
1)	Input Voltage:  PoE; 12 VDC. 
2)	Power Consumption:  22 W maximum.
3)	Power Connector:  2-position removable screw terminal block.
4)	Network Connector:  RJ-45 CAT 5.
5)	Audio Connector:  Screw terminal block.
6)	Alarm Input:  Screw terminal block.
7)	Video Out:  RJ-45 connector.
8)	Relay:  Screw terminal block.
9)	Radio Frequency Emission Rating:  FCC Class A.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 4 to 140 degrees F (minus 20 to 60 degrees C).
2)	Dimensions:
a)	Diameter:  7.2 inch (182.4 mm).
b)	Height:  8.2 inch (208.3 mm).
c)	Lower Dome:  4.3 inch (110 mm).
d)	Weight:  6.2 lbs (2.8 kg).
3)	Application:  Outdoor; IP66.
h.	Network Video Transmission:
1)	Compression:  H.265/H.264, M-JPEG.
2)	Video Output:  1920 x 1080 at 30 fps.
3)	Programming Interface:  ONVIF Profile S.
4)	Protocols:  IPv4/IPv6, HTTP, HTTPS, RTSP/RTP, RTCP, FTP, uPnP, TCP/IP, DHCP, UDP, ARP, QoS, Zeroconfig, Bonjour.
4.	Basis of Design:  SN683D-WIR Network PTZ Dome Camera as manufactured and supplied by Vicon Industries:
a.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
b.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
c.	Network Camera dome Features:
1)	Comprised of a camera/lens and pan/tilt drive in an attractive covert enclosure. Resolution:  3 MP.
2)	Network video transmission using either open platform H.265/H.264 or M-JPEG compression. ONVIF open architecture connectivity to enable third party software recording.
3)	Transmit high quality video across the network for remote viewing and recording and shall be configurable remotely from network digital video recorders and master workstations
4)	Four Alarm Inputs:  Programmable for functional state (enabled or disabled); can be set for Normally Open (NO) or Normally Closed (NC) and a dwell time programmable from 1 to 180 seconds.
5)	Alarm Output:  Able to control external equipment; able to be set for Normally Open (NO) or Normally Closed (NC). An audio alert available.
6)	Programmable Preset Positions:  256. Each preset has an individual title and is adjustable for pan and tilt speed and manual or auto focus.
7)	Tours:  8 with 64 presets per tour. Each tour has an individual title and is adjustable for pan, tilt and zoom speed and dwell time. Tours are programmable to repeat.
8)	Pan and Tilt Functions:  Programmable. Maximum Manual Pan and Tilt Speeds:  Programmable. Maximum Pan Speed:  380 degrees/sec and maximum tilt speed 380 degrees/sec. Pan and tilt speeds are scalable to the zoom setting. Pan Range:  360 degree continuous and tilt range is 100 degrees (minus 10 to 90 degrees).
9)	Camera/Lens:  3 MP 1/2.8-inch progressive scan CMOS true day/night (IR cut filter) with a 4.6-165 mm varifocal lens (optical 36x). True wide dynamic range (120 dB) to provide the highest quality image with excellent contrast.
10)	Synchronized IR illuminators with 1312 ft (400 m) range.
11)	High Level, Programmable Functions:
a)	Configuration via a web browser. 
b)	Dynamic adjustable bit rate. 
c)	Configurable brightness, sharpness and high-sensitivity. 
d)	Gain Control:  Adjustable. 
e)	Shutter Speed:  Programmable, automatic or manual. 
f)	White balance gain using red and blue scales. 
g)	Programmable backlight compensation or wide dynamic range. Horizontal flip shall be available. 
h)	Dynamic Noise Reduction control. 
i)	Video Content Analysis (VCA) provided for tampering, defog, digital image stabilization, face detection, line detector and field detector.
12)	PTZ Housing:  Die-cast aluminum; secured with tamperproof screws.
a)	Wall mount and a ceiling/pole mount to be available.
b)	Camera Dome Rating:  IP66 and IK10.
c)	Micro SD card slot for local storage.
13)	Event Map:  Available to establish a schedule for each event trigger from the camera. 15 events able to be registered.
14)	Privacy Masks:  16 programmable, available to hide certain areas for display on screen.
15)	Motion Detection:  16 configurable zones for motion detection. Each zone individually configurable for threshold, sensitivity and dwell time levels. 
16)	The capability to flip (invert) the video image to be available. This feature is useful when mounting units in an inverted position.
17)	Video transmission rate of 60 fps (50 fps PAL) dual stream or 30 fps (25 fps PAL) triple stream.
18)	Two-way audio.
19)	Simultaneous Viewing/Recording Streams per Camera:  10
d.	Network Video Transmission:
1)	Compression:  H.265/H.264, M-JPEG.
2)	Video Output:  3 MP at 30 fps.
3)	Protocols:  IPv4/IPv6, HTTP, HTTPS, RTSP/RTP, RTCP, QoS, FTP, TCP/IP, DHCP, UDP, uPnP, DDNS, Zeroconfig, Bonjour, ONVIF.
e.	Camera Specifications:
1)	Imaging Device:  1/2.8-inch progressive scan CMOS.
2)	Maximum Resolution:  3 MP (2048x1536).
** NOTE TO SPECIFIER **  Delete box camera paragraph if not required.
C.	Box Cameras:
** NOTE TO SPECIFIER **  Delete models not required.
1.	Basis of Design:  High Resolution Day/Night IP Indoor Box Camera as manufactured and supplied by Vicon Industries:
** NOTE TO SPECIFIER **  Delete models not required.
a.	Model IQB92WI-A5:  Motorized varifocal lens.
b.	Model IQB95NI-A6:  Motorized varifocal lens.
c.	Model HPOE-100:  PoE housing.
d.	Certifications:  CE, FCC Class A, ONVIF, PSIA, RoHS 2, UL, cUL
e.	General Features:
1)	Mounting:  1/4-20 mounting holes, top and bottom. 
** NOTE TO SPECIFIER **  Delete types not required.
2)	Lens:  No Lens. Accepts a CS-mount lens.
3)	Lens:  Camera/lens combination.
4)	Lens:  Motorized varifocal lens. integral 2.8 to -12 or 2.8 to 8.5 mm motorized zoom and focus.
5)	Day/night Operation:  Built-in IR-cut filter. 
6)	Wide Dynamic Range (WDR):  1 MP and 2 MP models.
7)	Simultaneous dual streaming video; H.264 and M-JPEG compression. 
8)	Two-way audio and on-camera microphone. 
9)	SD card slot for local storage.
10)	FCC Class A device. Supports ONVIF interface and PSIA. 
11)	Camera features:  AGC, BLC, white balance, automatic exposure, electronic shutter, flip and rotate 180 degrees, privacy masks, motion detection. Alarm I/O relay and analog video out.
f.	Camera Parameters:
1)	Imaging Device (2 MP):  1/2.7 inch.
2)	Imaging Device (5 MP):  1/3.2-inch.
3)	Resolution:  2 MP (1080p) and 5 MP models.
4)	Shutter Speed:  Auto, programmable, and fixed.
5)	Automatic Gain Control:  On/Off selectable.
6)	Sensitivity (2 MP):  Color:  0.1 lux. Black and White:  Below 0.05 lux. 
7)	Sensitivity (5 MP):  Color:  0.2 lux. Black and White:  Below 0.05 lux. 
8)	Adjustment, Tilt and Horizontal:  Dependent on mount
9)	Lens Adjustment:  Motorized zoom and focus, P-iris
10)	Focal Length:  2.8 to 12 mm or 2.8 to 8.5 mm varifocal
11)	Horizontal Field of View:  2.8 to 12 mm:  101 to 35 degrees. 2.8 to 8.5 mm:  93 to 44 degrees. 
g.	Physical Parameters:
1)	Operating Temperature:  32 to 113 degrees F (0 to 45 degrees C).
2)	Construction:  Aluminum and plastic.
3)	Dimensions H x W x L):  2.76 in (70.2 mm) x 2.72 in (69 mm) x 5.07 in (128.9 mm).
4)	Weight:  Approximately 0.4 lbs (0.165 kg).
h.	Electrical Parameters:
1)	Input Voltage:  PoE; 24 VAC, 12 VDC. Less than 4 W power consumption.
2)	Connectors, PoE:  RJ-45.
3)	Connectors, Video/Data:  RJ-45
4)	Connectors, I/O relay, audio in/out, analog output:  Push-in terminal.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
i.	Network Platforms:
1)	Communication Platform:  Open platform.
2)	Compression:  H.264; MPEG-4; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Multicast.
4)	Video Channels:  Dual streaming.
5)	Resolution, 1 MP, 720p:  1280 x 720.
6)	Resolution, 2 MP, 1080p:  1920 x 1080.
7)	Resolution, 5 MP:  2560 x 1920.
8)	Frame Rate, 2MP, (1080p):  30 fps.
9)	Frame Rate, 5 MP:  10 fps.
10)	Web Browser:  Internet Explorer, Firefox, Chrome, Safari, Mozilla, or Opera.
11)	Users:  10 user live viewing.
12)	Image Settings:  Configurable brightness, contrast, saturation, and sharpness. Auto exposure, auto white balance, AGC, BLC, motion detection, and AC lighting control (50 or 60 Hz)
13)	Supported Protocols:  IPV4, IPV6, TCP/IP, HTTP, HTTPS, RTSP, RTP, CIFS, SMTP, DHCP, NTP, DNS, UDP, uPnP, ARP, SNMP, ICMP, Zeroconf, APIPA, Telnet, and multicast.
2.	Basis of Design:  V2008-W-NL IP Box Camera as manufactured and supplied by Vicon Industries:
a.	Certifications:  CE, UL, FCC Class A, ONVIF S/T/G/Q, RoHS, NDAA/GSA/TSA compliant.
b.	l Features:
1)	Mounting:  1/4-20 mounting holes, top and bottom. 
** NOTE TO SPECIFIER **  Delete types not required.
2)	Lens:  DC iris.
3)	Lens:  P-iris.
4)	Lens:  i-CS.
5)	Day/night Operation:  Built-in IR-cut filter. 
6)	Wide Dynamic Range (WDR):  8 MP.
7)	Triple streaming video. 
8)	Camera features:  Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI, and motion detection.
c.	Camera Parameters:
1)	Imaging Device:  1/1.8 inch progressive scan.
2)	Maximum Resolution:  8 MP.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity:  Color:  0.02 lux. Black and White:  0.01 lux. 
6)	Adjustment, Tilt and Horizontal:  Dependent on mount
7)	Digital Zoom:  Dynamic ROI.
d.	Physical Parameters:
1)	Operating Temperature:  14 to 131 degrees F (minus 10 to 55 degrees C).
2)	Construction:  Aluminum and plastic.
3)	Dimensions, H x W x L:  2.4 in (62 mm) x 2.9 in (73 mm) x 4.1 in (104 mm).
4)	Weight:  Approximately 1.3 lbs (0.8 kg).
e.	Electrical Parameters:
1)	Input Voltage:  PoE; 24 VAC, 12 VDC. 
2)	Current:  PoE:  0.28 A; 12 VDC:  1.125 A; 24 VAC:  0.56 A.
3)	Power Consumption:  13.5 W.
4)	Connectors:
a)	Power:  24 VAC/12 VDC terminal block.
b)	PoE:  RJ-45.
c)	Video/Data:  RJ-45.
d)	Audio Input/Output:  terminal block; audio level alarm alert.
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
f.	Network Platforms:
1)	Communication Platform:  Open platform.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution:  3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
6)	Frame Rate:  Maximum 30 fps.
7)	Web Browser:  Internet Explorer, Firefox, Chrome, Safari, or Microsoft Edge.
8)	Users:  10 user live viewing.
9)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; dynamic ROI.
10)	Intelligent Video Analytics:  Tampering, Intelligent Motion Detection Intrusion Detection; Line Counter/Cross, Loitering, Object Left/Removed, Wrong Direction, Crowd Detection.
11)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
** NOTE TO SPECIFIER **  Delete specialty cameras paragraph if not required.
D.	Specialty Cameras:
** NOTE TO SPECIFIER **  Delete models not required.
1.	Basis of Design:  V-CELL-HD-B Corner Mounted HD Day/Night Cameras as manufactured by Vicon Industries:
** NOTE TO SPECIFIER **  UL and cUL certifications apply only if camera is supplied with back cover.
a.	Certifications:  CE, FCC Class A, IK10, IP66, UL, and cUL.
b.	Features:
1)	Made for custodial suites and prison cells.
2)	Mounting:  Stainless steel, waterproof housing. Fits into 90 degree corners. Fixed mounting frame and removable front plate. Assembly is permanently sealed to walls and ceiling making housing ligature proof. Front plate is recessed and secured to fixed frame with security screws. Two windows in front plate protect camera and IR LED illuminators. 
3)	Camera Mount:  Adjustable allowing for tilting up or down for an exact view.
4)	Alarms and audio. 
5)	Privacy masks.
c.	Camera Parameters:
1)	Imaging Device:  1/2.8-inch progressive scan RGB CMOS.
2)	Camera Type:  True day/night (IR cut filter)
3)	Sensitivity:  0.0 lux (IR On)
4)	IR Distance:  65 ft (20 m) with 36 IR LEDs. Programmable intensity.
5)	Lens Focal Length:  2.3 mm, fixed wide angle.
6)	Aperture:  f/2.0 maximum.
7)	Horizontal Field of View:  124 degrees.
8)	Vertical Field-of-View:  94 degrees.
d.	Physical Parameters:  
1)	Operating Temperature:  32 to 140 degrees F (0 to 60 degrees C).
2)	Application:  Indoor.
3)	Construction:  Enclosure:  Stainless steel; brushed satin. Mounting Frame:  14 gauge; camera mount:  14 gauge. Windows:  polycarbonate. IR:  5 mm thick. Camera:  6 mm thick. Dimensions:  15 in. (380 mm) x 12.6 in. (320 mm).
4)	Weight:  3.5 lbs (1.6 kg) approximate. Electrical Parameters:  
5)	Input Voltage/Current:  24 VAC 250 mA. 12 VDC 500 mA. PoE 125 mA.
6)	Power Consumption (IR on):  24 VAC:  6 W. 12 VDC:  6 W. PoE:  6 W.
7)	Connectors, 24 VAC and 12 VDC:  Screw terminal.
8)	Connectors, PoE:  RJ-45.
9)	Connectors, Alarms (In/Out) and Audio (mic/spkr):  Screw terminal. 
10)	Radio Frequency Emission Rating:  FCC Class A.
e.	Network Parameters:
1)	Compression:  H.264, MPEG-4 or M-JPEG and analog.
2)	Video Streams:  10 concurrent.
3)	Video Resolution:  2048x1536 (3 MP), 1920x1080 (Full HD 1080P), 1280x1024 (SXVGA), 1280x720 (HD 720P), 704x480/576 (D1), 640x480 (VGA), 352x240/288 (CIF), 320x240 (QVGA).
4)	Frame Rate:  Up to 30 fps.
5)	Video Bandwidth:  10/100 Mbps.
2.	Basis of Design:  V1110B-THM-TEMP Thermal Body Temperature Measurement Network Cameras as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	FCC, Class A.
3)	IP66.
4)	UL.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 2-year manufacturer warranty.
d.	Thermal Body Temperature Camera:
1)	Thermal camera shall provide for contactless measurement of people as they enter a facility. 
2)	Provides both a thermal camera and visible camera. 
3)	Includes a blackbody thermal detection unit that shall maintain calibration; it shall provide accuracy of plus or minus 0.54 degrees F (0.3 degrees C) for medical body temperature detection.
e.	Thermal and Visible Camera Specifications:
1)	Imaging Device:  Thermal Camera:  long-life uncooled IRFPA Microbolometer. Visible Camera:  1/2.8-inch CMOS.
2)	Max. Resolution:  Thermal Camera:  400 (H) x 300 (V) effective pixels. Visible Camera:  2 MP (1920x1080).
3)	Shutter Speed:  Visible Camera:  1/5 - 1/20,000 sec.
4)	Automatic Gain Control:  Yes (AGC).
5)	Sensitivity:  Thermal Camera:  40 mK at F1.0, 300K. Visible Camera:  Color:  0.1 lux; B&W:  0.01 lux at f/1.2, AGC On.
6)	Tilt and Horizontal:  Mount dependent.
7)	Digital Zoom:  Yes (ROI).
8)	Lens Adjustment:  Visible Camera:  Motorized lens.
9)	Focal Length:  Thermal Camera:  fixed 8 mm. Visible Camera:  2.7-12 mm varifocal.
10)	Field of View, Horizontal,  Thermal Camera:  46 degrees.
11)	Field of View, Vertical, Thermal Camera:  35 degrees.
12)	Field of View, Visible Camera:  105 to 32 degrees.
13)	Temperature Detection:  Body detection (supports 16 targets). Temperature Alarm for over temperature and temperature difference. Precision:  Plus or minus 0.54 degrees F (0.3 degrees C) with blackbody. Response Time:  Less than 30 ms. Pixel Pitch:  17 micrometers. Spectral range:  8 to 14 micrometers. Color palettes:  up to 17 modes (black-heat/white-heat/rainbow/iron-red).
f.	Blackbody Specifications:
1)	Temperature Range:  86 to 122 degrees F (30 to 50 degrees C).
2)	Emissive Area:  2.8 x 2.8 in. (72 x 72 mm).
3)	Temperature Resolution:  0.018 degrees F (0.01 degrees C).
4)	Accuracy:  Plus or minus 0.36 degrees F (0.2 degrees C).
5)	Stability:  Plus or minus 0.27 degrees F/10 min (0.15 degrees C/10 min).
6)	Emissivity:  0.97 plus or minus 0.02.
7)	Power Supply:  24 VDC; power supply included
8)	Operating Ambient Temperature:  32 to 104 degrees F (0 to 40 degrees C). 
9)	Dimensions:  7.1 x.4.3 x 4.3 in. (180 x 110 x 110 mm).
10)	Weight:  3.1 lb (1.4 kg).
g.	Electrical Specifications:  
1)	Input Voltage:  12 VDC or PoE.
2)	Current (IR on):  12 VDC:  0.83 A.
3)	Power Consumption (IR on):  10 W.
4)	Connectors:
a)	Power:  12 VDC connector or PoE RJ-45.
b)	Video/Data:  RJ-45.
c)	Alarm In/Out:  Screw terminal and jacks.
d)	Slot for Micro SD card.
e)	RS-485:  2-pin connector.
f)	Reset button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
h.	Physical Parameters:
1)	Operating Temperature:  Minus 22 to 140 degrees F (minus 30 to 60 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Metal.
4)	Dimensions:  
a)	Height:  5.4 inch (136 mm).
b)	Width:  7.2 inch (182 mm).
c)	Length:  8.3 inch (212 mm).
d)	Weight:  4.4 lbs (2 kg).
5)	Camera Mount:  Surface mount; wall or pendant, ceiling mount. Tripod mount available.
6)	Adjustments:  Mount allows positioning.
i.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus and ViconNet Video Management System or other ONVIF-based VMS.
2)	Compression:  H.264/H.265; M-JPEG.
3)	LAN Interface:  10/100 Base-T; one IP address for two channel.
4)	Resolution and Frame Rate:  Thermal Camera:  Main Stream:  D1; Sub-Stream:  CIF Visible Camera:  Main Stream:1920x1080 (2 MP), 280x720; Sub-Stream:  D1, VGA, 640x360, CIF, QVG, Max 30/25 fps.
5)	Web Browser:  Internet Explorer, Firefox, Chrome.
6)	Users:  Live viewing for up to 10 clients.
7)	Image Settings:  Mirror; configurable brightness, contrast, saturation, chroma, sharpness; AGC; Electronic Shutter; automatic or manual; digital zoom; motion detection; zoom and focus (motorized lens model)
8)	VCA:  Defog, Motion Detection, Line Cross (single and double), Object Left/Removed, Perimeter.
9)	Supported Protocols:  IPv4/IPv6, TCP/UDP, HTTP, RTSP, RTCP, RTP SIP, DHCP, SMTP, DNS, PPPOE, 802.1x.
** NOTE TO SPECIFIER **  Delete if not required.
E.	Dome Cameras:
** NOTE TO SPECIFIER **  Delete models not required.
1.	Basis of Design:  V1000-WIR-180-1 Series Multi-Sensor Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:
1)	CE
2)	FCC, Class A
3)	IP66
4)	IK10
5)	UL
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Outdoor Multi-Sensor Series Camera:
1)	Four camera/lens modules providing 1 180 degree panoramic view.
2)	Indoor/outdoor surface mounting.
a)	There shall be mounting accessories to allow wall mounting, pendant mounting, and an adapter to allow corner and pole mounting.
3)	High-resolution day/night camera; true WDR and IR capability and include four integral fixed lenses. 
4)	Day/Night Operation:  Achieved using a built-in IR-cut filter. IR distance shall be 90 ft (30 m).
5)	Camera Position:  Fixed position.
6)	Smart Encoding:  Monitors the amount of motion in a scene, resulting in overall savings in storage and bandwidth without sacrificing video quality.
7)	Powered by PoE or 24 VAC or 12 VDC.
8)	Triple streaming video and support H.264/H.265 compression. The camera modules shall have 1080p (2 megapixel) and 5 MP resolution, offering 8MP and 20 MP resolution models.
9)	Electronic iris, AGC, true WDR, white balance, backlight compensation, tampering, flip, mirror, privacy masks, ROI and motion detection.
10)	Meet FCC requirements for a Class A device. 
11)	Support for industry-standard ONVIF interface. IP66-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance.
12)	Slot for an SD card for local storage.
e.	Day/Night IP Dome Camera Specifications:
1)	Imaging Device:
a)	2 MP:  4x 1/2.7-inch progressive scan CMOS.
b)	5 MP:  4x 1/1.8-inch progressive scan CMOS.
2)	Max. Resolution:  4x 1920 x 1080 (2 MP) or 4x 2592 x 1944 (5 MP).
3)	Shutter Speed:  1/3.75 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity:
a)	2 MP:  Color:  0.05 lux; B&W:  0 lux (IR On) at f/1.8, 30 
b)	5 MP:  Color:  0.1 lux; B&W:  0 lux (IR On) at f/1.8
6)	Wide Dynamic Range:  True WDR, 120dB.
7)	Focal Length:
a)	2 MP:  4x 6.0 mm.
b)	5 MP:  4x 5.5 mm.
8)	Field of View:	
a)	2 MP:  Horiz:  180 degrees; Vert:  47 degrees.
b)	5 MP:  Horiz:  180 degrees; Vert:  32 degrees.
9)	IR Distance:  90 ft (30 m).
f.	Electrical Parameters:
1)	Input Voltage:  12 VDC or PoE, or 12 VAC.
2)	Current (IR on):  
a)	2 MP:  24 VAC:  0.8 A; 12 VDC:  1.7 A.
b)	5 MP:  24 VAC:  1.0 A; 12 VDC:  2.1 A.
3)	Power Consumption (IR on):  2 MP:  20 W; 5 MP:  25 W.
4)	Connectors:
a)	Pigtail :Power:  terminal block.
b)	PoE/Network:  RJ-45.
c)	Alarm:  terminal block.
d)	Audio:  phone jack.
e)	Slot for SD card.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 40 to 131 degrees F (minus 400 to 55 degrees C) 
2)	Humidity:  10 to 90 percent relative, non-condensing.
3)	Construction:  Die-cast aluminum housing; polycarbonate clear dome.
4)	Dimensions:  
a)	Height:  7.4 inch (188.4 mm).
b)	Diameter:  7.7 inch (196 mm).
c)	Weight:  Approximately 5.5 lb (2.5 kg).
5)	Camera Mount:  Surface mount.
h.	Network and Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus and ViconNet Video Management System.
2)	Compression:  H.264/H.265.
3)	LAN Interface:  10/100.
4)	Video Channels:  Triple streaming.
5)	Resolution:
6)	2 MP:  4x 1920x1080.
7)	5 MP:  4x 2592x1944.
8)	Frame Rate:  Max 30 fps at 8/20 MP
9)	Web Browser:  Internet Explorer, Safari, Firefox, Chrome.
10)	Users:  Live viewing for up to 10 clients.
11)	Image Settings:  Day/night mode; flip and mirror; configurable brightness, contrast, hue, sharpness, saturation; white balance, Gain Control; DNR; true WDR (120dB); privacy masks (5); motion detection; BLC; Exposure; ROI.
12)	Video Content Analytics:  Defog, Video Contents Analysis (Tampering); VMD.
13)	Supported Protocols:  IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTP, RTSP SMTP, FTP, UDP, uPnP, QoS, ICMP, SNMP, SSH, SSL, Zeroconfig DynDNS.
2.	Basis of Design:  V1020-WIR-360 Multi-Sensor Cameras as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP66, UL, and ONVIF S/G/Q/T.
b.	Features:
1)	Outdoor multi-sensor camera incorporating four camera or lens modules for a 360 degree panoramic view.
2)	True WDR and IR capability with four integral motorized lenses.
3)	Electronic iris, AGC, white balance, backlight compensation, tampering, flip, mirror, privacy masks and motion detection.
4)	Mounting:  Surface mountable. Wall, corner and pole mounting accessories available. 
c.	Camera Parameters:
1)	Imaging Device:  5 MP:  4x 1/2.8-inch progressive scan CMOS.
2)	Maximum Resolution:  4x 2592 x 1944, 5 MP.
3)	Shutter Speed:  1/7 - 1/20,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity:  Color:  0.03 lux; B&W:  0.01 (IR OFF), 0 lux (IR On) 
@30 IRE.
6)	Wide Dynamic Range:  True WDR, 120dB.
7)	Lens Focal Length:  4x 3.1-10 5 mm.
8)	Horizontal Field of View:  32 to 96 degrees.
9)	Vertical Field-of-View:  24 to 69 degrees.
10)	Field-of-View Depth:  40 to 124 degrees.
11)	IR Distance:  98 to 131 feet (29,870 to 39,930 mm).
d.	Physical Parameters:  
1)	Operating Temperature:  -40 to 131 degrees F (-40 to 55 degrees C).
2)	Operating Humidity:  10 to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Enclosure:  Die-cast aluminum housing. Dome:  Clear polycarbonate. Dimensions:  5.6 in. (142.3 mm) x 9.7 in. (247.5 mm) diameter.
5)	Weight:  5.2 lbs (2.36 kg) approximate. 
e.	Electrical Parameters:  
1)	Input Voltage/Current:  PoE+, 24 VAC, 24 VDC. 1.7 A.
2)	Power Consumption (IR on):  40 W.
3)	Connectors:  Pigtail:  Power:  terminal block.
4)	Connectors, PoE:  RJ-45.
5)	Connectors, Alarms (In/Out):  Terminal block. 
6)	Connectors, Audio:  Phone jack. 
7)	Connectors:  Slot for SD card. 
8)	Radio Frequency Emission Rating:  FCC Class A; CE.
f.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus and ViconNet Video Management Systems
2)	Compression:  H.264/H.265.
3)	LAN Interface:  Triple streaming.
4)	Video Resolution:  4x 2592x1944.
5)	Frame Rate:  Up to 30 fps.
1)	Web Browser:  Internet Explorer, Firefox, Google Chrome.
6)	Users:  Live viewing for up to 10 clients.
7)	Image Settings:  Day/night mode; flip and mirror; configurable brightness, contrast, hue, sharpness, saturation; white balance, gain control; DNR; true WDR (120dB); privacy masks (5); motion detection; BLC; Exposure; Audio.
8)	Video Content Analytics:  Video Contents Analysis:  Tampering; VMD; Intrusion Detection.
9)	Supported Protocols:  IPv4/IPv6, TCP/IP, HTTP, HTTPS, RTSP, RTP, RTCP SMTP, FTP, UDP, uPnP, QoS, ICMP, SNMP v2c/v3, SSL, DNS, NTP, LDAP (client), Zeroconfig, DynDNS, ONVIF S/G/Q/T.
3.	Basis of Design:  V2000D Outdoor IP Micro Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP66, UL, and ONVIF S/G/Q/T.
b.	Features:
1)	Outdoor fixed dome camera shall incorporate a fixed camera/lens combination.
2)	True WDR and Smart or Adaptive IR capability.
3)	Intelligent Video Analysis, tampering, intelligent motion detection, intrusion detection, line counting/cross, loitering, object left/removed, wrong direction and area counting.
4)	Mounting:  Surface mountable. 
c.	Camera Parameters:
1)	Imaging Device:  1/2.8-inch progressive scan.
** NOTE TO SPECIFIER **  Delete maximum resolution options not required.
1)	Maximum Resolution:  2 MP.
a)	Sensitivity:  Color:  0.007 lux; Black and White:  0.003 (IR OFF), 0 lux (IR On).
b)	Horizontal Field of View:  109 degrees.
c)	Vertical Field-of-View:  59 degrees.
d)	Field-of-View Depth:  128 degrees.
e)	Resolution:  1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
2)	Maximum Resolution:  5 MP.
a)	Sensitivity:  Color:  0.03 lux; Black and White:  0.01 (IR OFF), 0 lux (IR On).
b)	Horizontal Field of View:  104 degrees.
c)	Vertical Field-of-View:  78 degrees.
d)	Field-of-View Depth:  134 degrees.
e)	Resolution:  2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Digital Zoom:  Yes, ROI.
6)	Lens Adjustment:  Fixed.
7)	Lens Focal Length:  2.8 mm.
8)	IR Distance:  Smart IR/Adaptive IR; 49 ft (15 m) with 8 IR LEDs.
d.	Physical Parameters:  
1)	Operating Temperature:  Minus 4 to 131 degrees F (Minus 20 to 55 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum dome housing; polycarbonate clear dome. Dimensions:  2.2 in. (57 mm) x 4.3 in. (110 mm) diameter.
5)	Weight:  1.65 lbs (0.75 kg). 
e.	Electrical Parameters:  
1)	Input Voltage/Current:  PoE, 0.28A.
2)	Power Consumption, IR on:  13.5 W.
3)	Connectors:  
a)	Pigtail cable.
b)	PoE:  RJ-45.
c)	Video and Data:  RJ-45.
d)	Audio:  Screw terminal, audio level alarm alert. 
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
4)	Radio Frequency Emission Rating:  FCC Class A; CE.
f.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Frame Rate:  Up to 30 fps.
5)	Web Browser:  Internet Explorer, Safari, Firefox, Google Chrome, Microsoft Edge.
6)	Users:  Live viewing for up to 10 clients.
7)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
8)	Intelligent Video Analytics:  Tampering/Defocus, Intelligent Motion Detection, Intrusion Detection; Line Counter/Cross, Loitering, Object Left/Removed, Wrong Direction, Area Counting.
9)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
4.	Basis of Design:  V2000D Outdoor IP Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP67, UL, RoHS, ONVIF S/G/Q/T and NDAA/GSA/TSA compliant.
b.	Features:
1)	Outdoor fixed dome camera shall incorporate a fixed camera/lens combination.
2)	True WDR and Smart or Adaptive IR capability.
3)	Intelligent Video Analysis, tampering, intelligent motion detection, intrusion detection, line counting/cross, loitering, object left/removed, wrong direction and area counting.
4)	Mounting:  Surface mountable. 
c.	Camera Parameters:
** NOTE TO SPECIFIER **  Delete maximum resolution options not required.
1)	Maximum Resolution:  2 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity:  Color:  0.007 lux; Black and White:  0.002 (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  110 to 34 degrees.
d)	Vertical Field-of-View:  58 to 20 degrees.
e)	Field-of-View Depth:  134 to 40 degrees.
f)	Resolution:  1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
g)	Lens Focal Length:  3.1 to 10 mm varifocal.
h)	Current:  PoE:  0.24 A; 24 VAC:  0.48 A; 12 VDC:  0.96 A.
i)	Power Consumption IR and Heaters On:  11.52 W.
2)	Maximum Resolution:  5 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity:  Color:  0.03 lux; Black and White:  0.01 (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  96 to 32 degrees.
d)	Vertical Field-of-View:  69 to 24 degrees.
e)	Field-of-View Depth:  124 to 40 degrees.
f)	Resolution:  2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180.
g)	Lens Focal Length:  3.1 to 10 mm varifocal.
h)	Current:  PoE:  0.3 A; 24 VAC:  0.6 A; 12 VDC:  1.2 A.
i)	Power Consumption IR and Heaters On:  14.4 W.
3)	Maximum Resolution:  8 MP.
a)	Imaging Device:  1/1.8-inch progressive scan.
b)	Sensitivity:  Color:  0.02 lux; Black and White:  0.01 (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  96 to 46 degrees.
d)	Vertical Field-of-View:  54 to 26 degrees.
e)	Field-of-View Depth:  113 to 54 degrees.
f)	Resolution:  3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
g)	Lens Focal Length:  3.6 to 10 mm varifocal.
h)	Current:  PoE:  0.27 A; 24 VAC:  0.55 A; 12 VDC:  1.1 A.
i)	Power Consumption IR and Heaters On:  13.14 W.
4)	Shutter Speed:  1/2 - 1/10,000 sec.
5)	Automatic Gain Control:  On/Off selectable.
6)	Digital Zoom:  Yes, ROI.
7)	Tilt and Horizontal:  Three-direction adjustment, allowing for adjustment of pan, tilt and lens rotation.
8)	Lens Adjustment:  Motorized lens, P-iris automatically adjusts to zoom condition.
9)	IR Distance:  Smart IR/Adaptive IR; 131 ft (40 m) with 22 IR LEDs.
d.	Physical Parameters:  
1)	Operating Temperature:  Minus 40 to 140 degrees F (Minus 40 to 60 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum alloy body; polycarbonate clear dome. Dimensions:  4.49 in. (125 mm) x 5.3 in. (135 mm) diameter.
5)	Weight:  2.6 (1.2 kg). 
e.	Electrical Parameters:  
1)	Input Voltage:  24 VAC, 12 VDC or PoE.
2)	Connectors:  
a)	Two conduit access holes for internal cable termination.
b)	Power:  12 VDC or 24 VAC terminal block.
c)	PoE:  RJ-45.
d)	Video and Data:  RJ-45.
e)	Alarm:  Screw terminal.
f)	Audio:  Screw terminal, audio level alarm alert. 
g)	Slot for SD card.
h)	Composite output for installation-2-pin connector.
i)	Reset button.
j)	Default button.
3)	Radio Frequency Emission Rating:  FCC Class A; CE.
f.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Frame Rate:  Up to 30 fps.
6)	Web Browser:  Internet Explorer, Safari, Firefox, Google Chrome, Microsoft Edge.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
9)	Intelligent Video Analytics:  Tampering/Defocus, Intelligent Motion Detection, Intrusion Detection; Line Counter/Cross, Loitering, Object Left/Removed, Wrong Direction, Area Counting.
10)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
5.	Basis of Design:  V2100D Outdoor IP Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP67, UL, RoHS, ONVIF S/G/Q/T and NDAA/GSA/TSA compliant.
b.	Features:
1)	Outdoor dome camera shall incorporate a fixed camera/lens combination.
2)	True WDR and Smart IR capability.
3)	Intelligent Video Analysis, motion and tampering/defocus.
4)	Mounting:  Surface mountable. 
c.	Camera Parameters:
** NOTE TO SPECIFIER **  Delete maximum resolution options not required.
1)	Maximum Resolution:  2 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity:  Color:  0.015 lux; Black and White:  0.005 (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  102 to 34 degrees.
d)	Vertical Field-of-View:  54 to 20 degrees.
e)	Field-of-View Depth:  118 to 40 degrees.
f)	Resolution:  1920x1080, 1280x960/720, 800x600, 640x480.
2)	Maximum Resolution:  5 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity:  Color:  0.05 lux; Black and White:  0.03 (IR OFF), 0 lux (IR On).
c)	Horizontal Field of View:  96 to 32 degrees.
d)	Vertical Field-of-View:  69 to 24 degrees.
e)	Field-of-View Depth:  124 to 40 degrees.
f)	Resolution:  2592x1944/1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Digital Zoom:  Yes, ROI.
6)	Tilt and Horizontal:  Two-direction adjustment, allowing for adjustment of pan and tilt.
7)	Lens Adjustment:  Motorized lens, DC-iris.
8)	IR Distance:  Smart IR; 98 ft (30 m) with 16 IR LEDs.
d.	Physical Parameters:  
1)	Operating Temperature:  Minus 22 to 140 degrees F (Minus 30 to 60 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum alloy body; bracket:  PC+ABS; window:  double glass/polycarbonate clear dome. 
5)	Dimensions:  4.4 in. (112 mm) x 5.3 in. (135 mm) diameter.
6)	Weight:  2.2 (1 kg). 
e.	Electrical Parameters:  
1)	Input Voltage:  12 VDC or PoE.
2)	Current:  PoE:  0.16 A; 12 VDC:  0.63 A.
3)	Power Consumption IR On:  7.6 W.
4)	Connectors:  
a)	Power:  12 VDC terminal block.
b)	PoE:  RJ-45.
c)	Video and Data:  RJ-45.
d)	Slot for SD card.
e)	Reset button.
f)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
f.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Frame Rate:  Up to 30 fps.
6)	Web Browser:  Internet Explorer, Safari, Firefox, Google Chrome, Microsoft Edge.
7)	Users:  Live viewing for up to 10 clients.
8)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
9)	Intelligent Video Analytics:  Tampering/Defocus, Motion.
10)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
6.	Basis of Design:  V2360W Outdoor IP Panoramic Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:  CE, FCC Class A, IK10, IP67, UL, RoHS, ONVIF S/G/Q/T and NDAA/GSA/TSA compliant.
b.	Features:
1)	Outdoor panoramic dome camera shall incorporate a fixed camera/lens combination.
2)	True WDR and Smart IR capability.
3)	Intelligent Video Analysis, motion and tampering/defocus.
4)	Mounting:  Surface mountable. 
c.	Camera Parameters:
1)	Imaging Device:  1/1.7-inch.
2)	Maximum Resolution:  12 MP.
3)	Shutter Speed:  1/2 - 1/10,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity:  Color:  0.04 lux; Black and White:  0.03 (IR OFF), 0 lux (IR On).
6)	Digital Zoom:  Dynamic ROI.
7)	Lens Adjustment:  Fixed fisheye.
8)	Focal Length:  1.2 mm.
9)	Field of View:  195 degrees, 360 degree surround view.
10)	IR Distance:  Smart IR; 49 ft (15 m) with 1 IR LED.
11)	Dual heater system.
d.	Physical Parameters:  
1)	Operating Temperature:  Minus 40 to 122 degrees F (Minus 40 to 50 degrees C).
2)	Operating Humidity:  Up to 90 percent relative, non-condensing.
3)	Application:  Indoor or Outdoor.
4)	Construction:  Aluminum alloy body; bracket:  PC+ABS front case. 
5)	Dimensions:  2.2 in. (57 mm) x 5 in. (150 mm) diameter.
6)	Weight:  2 (0.9 kg). 
e.	Electrical Parameters:  
1)	Input Voltage:  24 VAC or PoE.
2)	Current:  PoE:  0.52 A; 24 VAC:  1.1 A.
3)	Power Consumption IR On:  25 W.
4)	Connectors:  
a)	Power:  24 VAC terminal block.
b)	PoE:  RJ-45.
c)	Video and Data:  RJ-45.
d)	Audio In and Out:  Screw terminal; built-in mic; audio level alarm alert.
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
f.	Network Parameters:
1)	Communications:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
5)	Resolution:  4000x3000, 3000x3000, 2592x1944, 1944x1944, 048x1536, 1536x1536, 1280x960, 960x960, 800x600, 608x600, 640x480, 480x480, 230x240, 240x240.
6)	Frame Rate:  Up to 30 fps.
7)	Web Browser:  Internet Explorer, Safari, Firefox, Google Chrome, Microsoft Edge.
8)	Users:  Live viewing for up to 10 clients.
9)	Image Settings:  Digital image effects defog, flip; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; dynamic ROI.
10)	Intelligent Video Analytics:  Tampering/Defocus, Motion.
11)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, FTP, HLS, ICMP, IGMP, LDAP, NTP, DHCP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
** NOTE TO SPECIFIER **  Delete if not required.
F.	Bullet Cameras:
** NOTE TO SPECIFIER **  Delete models not required.
1.	Basis of Design:  V922B-W551MIR-A1 Outdoor IP Bullet Cameras as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	FCC, Class A.
3)	IP66.
4)	IK10.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Outdoor IP Bullet Camera:
1)	Fixed camera/lens combination. 
2)	Indoor/outdoor surface mounting. 
3)	High-resolution day/night camera;  true WDR and IR capability and include an integral 5 to 51 mm varifocal auto iris lens. 
4)	Motorized Lens:  Allow for remote configuration of zoom and focus (motorized focus and zoom). 
5)	Day/Night Operation:  Achieved using a built-in IR-cut filter. IR distance shall be 82 ft (25 m) with 32 IR LEDs. 
6)	Camera Position:  Adjustable using the integral mount. Sunshield provided.
7)	Powered by PoE Plus or 12 VDC. 
8)	Heater provided. 
9)	Triple streaming video and support H.264 and M-JPEG compression. The camera to be available in 1080p (2 megapixel) resolution.
10)	Electronic iris, AGC, BLC, white balance, flip, mirror and motion detection.
11)	Meet the FCC requirements for a Class A device. Include support for the industry-standard ONVIF interface. It shall be IP66-rated to withstand rain, dust and vandalism and IK10 rated for impact resistance.
12)	Provide a slot for an SD card for local storage.
13)	Meet or exceed the following design and performance specifications. 
e.	Day/Night IP Bullet Camera Specifications:
1)	Imaging Device:  1/2.8-inch progressive scan RGB CMO.
2)	Max. Resolution:  1080p.
3)	Shutter Speed:  1/3 to 1/30,000 sec.
4)	Automatic Gain Control:  On/Off selectable.
5)	Sensitivity:  Color:  0.35 lux; Black and White:  0.013 lux;  at 50 IRE.
6)	Tilt and Horizontal Integral mount allows positioning adjustment.
7)	Digital Zoom:  Yes (ROI).
8)	Lens Adjustment:  Motorized lens, iris automatically adjusts to zoom condition.
9)	Focal Length:  5 to 51 mm varifocal.
10)	Horizontal Field of View:  54 to 4.9 degrees.
11)	IR Distance:  82 ft (25m) with 32 IR LEDs.
f.	Electrical Specifications:  
1)	Input Voltage:  12 VDC or PoE Plus.
2)	Current (IR on):  PoE:  0.47 A; 12 VDC:  1.6 A, IR on.
3)	Power Consumption (IR on):  PoE:  22.6 W;  12 VDC:  19.2 W, IR/heater on.
4)	Connectors:
a)	Power:  12 VDC jack or E RJ-45.
b)	Video/Data:  RJ-45.
c)	Alarm:  screw terminal.
d)	Audio:  screw terminal.
e)	Slot for uSD card.
f)	Composite output for installation on camera board.
g)	Reset button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  minus 22 to 122 degrees F (minus 30 to 50 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Die-cast aluminum. Tamperproof screws.
4)	Dimensions:  
a)	Height:  3.7 inch (92.9 mm).
b)	Width:  3.9 inch (98.4 mm).
c)	Depth:  11.4 inch (289.5 mm), including sunshield and mount.
d)	Weight:  Approximately 2.3 lbs (1.04 kg).
5)	Camera Mount:  Surface mount.
6)	Adjustments:  Integral mount allows positioning.
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus and ViconNet Video Management System.
2)	Compression:  H.264; MPEG-4; M-JPEG available on 2nd stream.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Dual/triple streaming.
5)	Resolution and Frame Rate:  1920x1080, 1280x720, 704x480/576, 352x240/288, 640x480, 320x240; Max 60 fps at 1920x1080.
6)	Web Browser:  Internet Explorer, Safari, Firefox, Chrome.
7)	Users:  Live viewing for up to 10 clients; playback 3 clients.
8)	Image Settings:  Adjustable bit rate; flip and mirror; configurable brightness, contrast, hue, sharpness; white balance, AGC; Electronic Shutter; automatic or manual; BLC; digital zoom; motion detection; zoom and focus (motorized lens models).
9)	Supported Protocols:  IPv4/IPv6, TCP/IP, HTTP, HTTPS RTSP, RTCP, RTP SMTP, DHCP, NTP, FTP DDNS, UDP, uPnP,QoS, ARP, Bonjour, Zeroconf, Manual.
2.	Basis of Design:  V1100B-THM Temperature Detection Thermal Bullet Network Cameras as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	FCC, Class A.
3)	IP66.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Thermal Bullet Network Camera:
1)	Temperature detection thermal bullet cameras shall create images based on the heat that radiates from a person or object. 
2)	Configurable for either a standalone or integrated system. 
e.	Thermal Bullet Network Camera Specifications:
1)	Imaging Device:  Long-life uncooled IRFPA Microbolometer Vox sensing mode.
2)	Max. Resolution:  400 horizontal x 300 vertical effective pixels.
3)	Sensitivity:  Thermal Camera:  40 mK @F1.0, 300K.
4)	Tilt and Horizontal Integral mount allows positioning adjustment.
5)	Digital Zoom:  Yes.
** NOTE TO SPECIFIER **  Delete lens options not required.
6)	Lens:  15 mm:
a)	Field of View, Horizontal:  25.5 degrees.
b)	Field of View, Vertical:  19.2 degrees.
c)	Temperature Detection Distance, Fire-Body:  1447 feet (441 m).
d)	Temperature Detection Distance, Vehicle:  4439 feet (1353 m).
e)	Recognition Distance, Body:  361 feet (110 m).
f)	Recognition Distance, Vehicle:  1109 feet (338 m).
g)	Recognition Distance, Fire:  482 feet (147 m).
7)	Lens:  25 mm:
a)	Field of View, Horizontal:  15.4 degrees.
b)	Field of View, Vertical:  11.6 degrees.
c)	Temperature Detection Distance, Fire-Body:  2411 feet (735 m).
d)	Temperature Detection Distance, Vehicle:  7398 feet (2255 m).
e)	Recognition Distance, Body:  604 feet (184 m).
f)	Recognition Distance, Vehicle:  1850 feet (564 m).
g)	Recognition Distance, Fire:  804 feet (245 m).
8)	Lens:  35 mm:
a)	Field of View, Horizontal:  11 degrees.
b)	Field of View, Vertical:  8.3 degrees.
c)	Temperature Detection Distance, Fire-Body:  3376 feet (1029 m).
d)	Temperature Detection Distance, Vehicle:  10292 feet (3137 m).
e)	Recognition Distance, Body:  843 feet (257 m).
f)	Recognition Distance, Vehicle:  2589 feet (789 m).
g)	Recognition Distance, Fire:  1125 feet (343 m).
9)	Lens:  50 mm:
a)	Field of View, Horizontal:  7.7 degrees.
b)	Field of View, Vertical:  5.8 degrees.
c)	Temperature Detection Distance, Fire-Body:  4826 feet (1471 m).
d)	Temperature Detection Distance, Vehicle:  14,797 feet (4510 m).
e)	Recognition Distance, Body:  1207 feet (368 m).
f)	Recognition Distance, Vehicle:  3698 feet (1127 m).
g)	Recognition Distance, Fire:  1608 feet (490 m).
10)	Focal Length:  F/1.0.
f.	Electrical Specifications:  
1)	Input Voltage:  12 VDC, 24 VAC, or PoE.
2)	Current (IR on):  12 VDC:  0.42 A; 24 VAC:  0.20 A.
3)	Power Consumption (IR on):  5 W max.
4)	Connectors:
a)	Power:  12 VDC/24 VAC connector.
b)	PoE /Network:  RJ-45.
c)	Alarm In/Out:  Screw terminal and jacks.
d)	Slot for Micro SD card.
e)	RS-485:  2-pin connector.
f)	Reset button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 40 to 140 degrees F (minus 40 to 60 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Aluminum.
4)	Dimensions:  
a)	Length:  15.3 inch (388 mm).
b)	Diameter:  4.35 inch (110 mm).
c)	Weight:  4.2 lbs (1.9 kg).
5)	Camera Mount:  Surface mount; integral wall mount. Pole mount and junction box optional accessories.
6)	Adjustments:  Integral mount allows positioning.
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus and ViconNet Video Management System or other ONVIF-based VMS.
2)	Compression:  H.264/H.265; M-JPEG.
3)	LAN Interface:  10/100 Base-T.
4)	Resolution and Frame Rate:  Main stream:  D1; Sub-Stream:  CIF. Unicast. 400x300effective pixels, Max 30/25 fps.
5)	Web Browser:  Internet Explorer, Firefox, Chrome.
6)	Users:  Live viewing for up to 10 clients.
7)	Image Settings:  Mirror; configurable brightness, contrast, sharpness; ROI; FFC; DNR (3D); digital zoom; privacy masking; image correction; image color mode; polarity/LUT; temperature measurement and parameters; Alarm triggers including temperature alarm, motion detection; I/O alarm, network disconnect, disk alarm.
8)	VCA:  Line Cross (single and double), Loitering, Tampering, Object Left/Removed, Perimeter, Abnormal Speed, Directional Motion, Illegal Parking.
9)	Supported Protocols:  IPv4/IPv6, TCP/UDP, HTTP, RTSP, RTCP, RTP FTP DHCP, SMTP, DNS, DDNS, PPPOE, SIP.
3.	Basis of Design:  V2000B Outdoor IP Bullet Cameras as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	UL.
3)	FCC, Class A.
4)	IP67.
5)	IK10, including front glass.
6)	ONVIF S/T/G/Q.
7)	RoHS.
8)	NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Outdoor IP Bullet Camera:
1)	Fixed camera/lens combination. 
2)	Indoor/outdoor surface mounting. 
3)	High-resolution day/night camera; true WDR and Smart IR/Adaptive IR capability and include an integral varifocal DC-iris lens. 
4)	Motorized Lens:  Allow for remote configuration of zoom and focus (motorized focus and zoom). 
5)	Day/Night Operation:  Achieved using a built-in IR-cut filter.
6)	Camera Position:  Adjustable using the integral mount. Sunshield provided.
7)	Dual heater provided. 
8)	Triple streaming video and support H.264/H.265 and M-JPEG compression. 
9)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
e.	Day/Night IP Bullet Camera Specifications:
** NOTE TO SPECIFIER **  Delete maximum resolution options not required.
1)	Max. Resolution:  2 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity at 30 IRE:  Color:  0.007 lux; black and white:  0.002 lux/0 lux (IR Off/On).
c)	Focal Length:  3.1 to 10 mm varifocal.
d)	Horizontal Field of View:  110 to 34 degrees.
e)	Vertical Field of View:  58 to 20 degrees.
f)	Depth Field of View:  134 to 40 degrees.
g)	Current:  PoE:  0.39 A; 24 VAC:  0.78 A; 12 VDC:  1.56 A.
h)	Power Consumption, IR On:  18.72 W.
2)	Max. Resolution:  5 MP.
a)	Imaging Device:  1/2.8-inch progressive scan.
b)	Sensitivity at 30 IRE:  Color:  0.03 lux; black and white:  0.01 lux/0 lux (IR Off/On).
c)	Focal Length:  3.1 to 10 mm varifocal.
d)	Horizontal Field of View:  96 to 32 degrees.
e)	Vertical Field of View:  69 to 24 degrees.
f)	Depth Field of View:  124 to 40 degrees.
g)	Current:  PoE:  0.42 A; 24 VAC:  0.83 A; 12 VDC:  1.67 A.
h)	Power Consumption, IR On:  20 W.
3)	Max. Resolution:  8 MP.
a)	Imaging Device:  1/1.8-inch progressive scan.
b)	Sensitivity at 30 IRE:  Color:  0.02 lux; black and white:  0.01 lux/0 lux (IR Off/On).
c)	Focal Length:  3.6 to 10 mm varifocal.
d)	Horizontal Field of View:  98 to 46 degrees.
e)	Vertical Field of View:  54 to 26 degrees.
f)	Depth Field of View:  113 to 54 degrees.
g)	Current:  PoE:  0.41 A; 24 VAC:  0.82 A; 12 VDC:  1.64 A.
h)	Power Consumption, IR On:  19.68 W.
4)	Shutter Speed:  1/2 - 1/10,000 sec.
5)	Tilt and Horizontal:  Three-direction adjustment, allowing for adjustment of pan, tilt and rotation.
6)	Digital Zoom:  Yes (ROI).
7)	Lens Adjustment:  Motorized lens, P-iris automatically adjusts to zoom condition.
8)	IR Distance:  Smart IR/Adaptive IR; 131 ft (40 m) with 4 IR LEDs.
f.	Electrical Specifications:  
1)	Input Voltage:  24 VAC, 12 VDC or PoE Plus.
2)	Connectors:
a)	Power:  12 VDC or 24 VAC terminal block.
b)	PoE:  RJ-45.
c)	Video/Data:  RJ-45.
d)	Alarm:  Screw terminal.
e)	Audio:  Screw terminal.
f)	Slot for SD card.
g)	Reset button.
h)	Default button.
3)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 40 to 140 degrees F (minus 40 to 60 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Aluminum alloy body; sunshield:  PC+ABS.
4)	Dimensions:  
a)	Length:  10.3 inch (261 mm).
b)	Diameter:  3.5 inch (89 mm).
c)	Weight:  4 lbs (1.8 kg).
5)	Camera Mount:  Surface mount.
6)	Adjustments:  Integral mount allows positioning.
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
** NOTE TO SPECIFIER **  Delete resolution options not required.
5)	Resolution, 2 MP:  1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
6)	Resolution, 5 MP:  2592x1944/1520, 2560x1440, 2048x1536, 2304x1296, 1920x1080, 1600x1200, 1440x1080, 1600x900, 1280x960/720, 800x600, 640x480, 640x360, 320x240, 320x180.
7)	Resolution, 8 MP:  3840x2160, 3264x1840, 2592x1944, 2688x1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480, 640x360, 320x240.
8)	Frame Rate:  Max 30 fps.
9)	Web Browser:  Internet Explorer, Safari, Firefox, Chrome, Microsoft Edge.
10)	Users:  Live viewing for up to 10 clients.
11)	Image Settings:  Digital image effects defog, flip and mirror; configurable, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
12)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
4.	Basis of Design:  V2100B Outdoor IP Bullet Cameras as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	UL.
3)	FCC, Class A.
4)	IP67.
5)	IK08.
6)	ONVIF S/T/G/Q.
7)	RoHS.
8)	NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Outdoor IP Bullet Camera:
1)	Fixed camera/lens combination. 
2)	Indoor/outdoor surface mounting. 
3)	High-resolution day/night camera; true WDR and Smart IR capability and include an integral varifocal DC-iris lens. 
4)	Motorized Lens:  Allow for remote configuration of zoom and focus (motorized focus and zoom). 
5)	Day/Night Operation:  Achieved using a built-in IR-cut filter.
6)	Camera Position:  Adjustable using the integral mount. 
7)	Triple streaming video and support H.264/H.265 and M-JPEG compression. 
8)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
e.	Day/Night IP Bullet Camera Specifications:
1)	Imaging Device:  1/2.8-inch progressive scan.
** NOTE TO SPECIFIER **  Delete maximum resolution options not required.
2)	Maximum Resolution:  2 MP.
a)	Sensitivity at 30 IRE:  Color:  0.015 lux; black and white:  0.01 lux/0 lux (IR Off/On).
b)	Horizontal Field of View:  102 to 34 degrees.
c)	Vertical Field of View:  54 to 20 degrees.
d)	Depth Field of View:  118 to 40 degrees.
3)	Maximum Resolution:  5 MP.
a)	Sensitivity at 30 IRE:  Color:  0.05 lux; black and white:  0.03 lux/0 lux (IR Off/On).
b)	Horizontal Field of View:  96 to 32 degrees.
c)	Vertical Field of View:  69 to 24 degrees.
d)	Depth Field of View:  124 to 40 degrees.
4)	Shutter Speed:  1/2 - 1/10,000 sec.
5)	Automatic Gain Control:  On/Off selectable.
6)	Tilt and Horizontal:  Two-direction adjustment, allowing for adjustment of pan and tilt.
7)	Digital Zoom:  Yes (ROI).
8)	Lens Adjustment:  Motorized lens, DC-iris .
9)	Focal Length:  3.1 to 10 mm varifocal.
10)	IR Distance:  Smart IR; 98 ft (30 m) with 16 IR LEDs.
f.	Electrical Specifications:  
1)	Input Voltage:  12 VDC or PoE.
2)	Current:  PoE:  0.16 A; 12 VDC:  0.63 A.
3)	Power Consumption:  IR On:  7.6 W; IR Off:  5.2 W.
4)	Connectors:
a)	Pigtail cable provided.
b)	Power:  12 VDC terminal block.
c)	PoE:  RJ-45.
d)	Video/Data:  RJ-45.
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 22 to 140 degrees F (minus 30 to 60 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Aluminum alloy body; bracket:  PC+ABS; window:  double glass/polycarbonate.
4)	Dimensions:  
a)	Length:  6.9 inch (177 mm).
b)	Width:  3.3 inch (84 mm).
c)	Height:  3.1 inch (79 mm).
d)	Weight:  2 lbs (0.9 kg).
5)	Camera Mount:  Surface mount.
6)	Adjustments:  2-axis camera adjustment.
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
** NOTE TO SPECIFIER **  Delete resolution options not required.
5)	Resolution, 2 MP:  1920x1080, 1280x960/720, 800x600, 640x480.
6)	Resolution, 5 MP:  2592x1944/1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480.
7)	Frame Rate:  Max 30 fps.
8)	Web Browser:  Internet Explorer, Safari, Firefox, Chrome, Microsoft Edge.
9)	Users:  Live viewing for up to 10 clients.
10)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
11)	Video Content Analysis:  Tampering/defocus, motion.
12)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
5.	Basis of Design:  V2100B Outdoor IP Mini Bullet Cameras as manufactured by Vicon Industries:
a.	Certifications:  
1)	CE.
2)	UL.
3)	FCC, Class A.
4)	IP67.
5)	IK08.
6)	ONVIF S/T/G/Q.
7)	RoHS.
8)	NDAA/GSA/TSA compliant.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Outdoor IP Bullet Camera:
1)	Fixed camera/lens combination. 
2)	Indoor/outdoor surface mounting. 
3)	High-resolution day/night camera; true WDR and Smart IR capability and include an integral fixed lens. 
4)	Day/Night Operation:  Achieved using a built-in IR-cut filter.
5)	Camera Position:  Adjustable using the integral mount. 
6)	Triple streaming video and support H.264/H.265 and M-JPEG compression. 
7)	Electronic iris, AGC, TWDR, white balance, defog, flip, mirror, privacy masking, ROI and motion detection.
e.	Day/Night IP Bullet Camera Specifications:
1)	Imaging Device:  1/2.8-inch progressive scan.
** NOTE TO SPECIFIER **  Delete maximum resolution options not required.
2)	Maximum Resolution:  2 MP.
a)	Sensitivity at 30 IRE:  Color:  0.015 lux; black and white:  0.01 lux/0 lux (IR Off/On).
b)	Horizontal Field of View:  110 degrees.
c)	Vertical Field of View:  60 degrees.
d)	Depth Field of View:  130 degrees.
3)	Maximum Resolution:  5 MP.
a)	Sensitivity at 30 IRE:  Color:  0.09 lux; black and white:  0.07 lux/0 lux (IR Off/On).
b)	Horizontal Field of View:  97 degrees.
c)	Vertical Field of View:  71 degrees.
d)	Depth Field of View:  126 degrees.
4)	Shutter Speed:  1/2 - 1/10,000 sec.
5)	Automatic Gain Control:  On/Off selectable.
6)	Tilt and Horizontal:  Two-direction adjustment, allowing for adjustment of pan and tilt.
7)	Digital Zoom:  Yes (ROI).
8)	Lens Adjustment:  Fixed.
9)	Focal Length:  2.8 mm.
10)	IR Distance:  Smart IR; 98 ft (30 m) with 16 IR LEDs.
f.	Electrical Specifications:  
1)	Input Voltage:  12 VDC or PoE.
2)	Current:  PoE:  0.14 A; 12 VDC:  0.56 A.
3)	Power Consumption:  IR On:  6.7 W; IR Off:  4.3 W.
4)	Connectors:
a)	Pigtail cable provided.
b)	Power:  12 VDC terminal block.
c)	PoE:  RJ-45.
d)	Video/Data:  RJ-45.
e)	Slot for SD card.
f)	Reset button.
g)	Default button.
5)	Radio Frequency Emission Rating:  FCC Class A; CE.
g.	Physical Parameters:
1)	Operating Temperature:  Minus 22 to 140 degrees F (minus 30 to 60 degrees C) with heater.
2)	Humidity:  Up to 90 percent relative, non-condensing.
3)	Construction:  Aluminum alloy body; bracket:  PC+ABS; window:  double glass/polycarbonate.
4)	Dimensions:  
a)	Length:  5.8 inch (147 mm).
b)	Width:  3.3 inch (84 mm).
c)	Height:  3.1 inch (79 mm).
d)	Weight:  1.8 lbs (0.8 kg).
5)	Camera Mount:  Surface mount.
6)	Adjustments:  2-axis camera adjustment.
h.	Network Video Specifications:
1)	Communication Platform:  Open platform; compatible with Valerus Video Management System.
2)	Compression:  Smart Encoding; H.264/H.265; M-JPEG.
3)	LAN Interface:  10 Base-T/100 Base-TX, Unicast/Multicast.
4)	Video Channels:  Triple streaming.
** NOTE TO SPECIFIER **  Delete resolution options not required.
5)	Resolution, 2 MP:  1920x1080, 1280x960/720, 800x600, 640x480.
6)	Resolution, 5 MP:  2592x1944/1520, 2048x1536, 1920x1080, 1280x960/720, 800x600, 640x480.
7)	Frame Rate:  Max 30 fps.
8)	Web Browser:  Internet Explorer, Safari, Firefox, Chrome, Microsoft Edge.
9)	Users:  Live viewing for up to 10 clients.
10)	Image Settings:  Digital image effects defog, flip and mirror; configurable brightness, contrast, saturation, hue, sharpness; BLC; HLC; gamma correction; 3 DNR; motion detection; white balance, AGC; Electronic Shutter, automatic or manual; digital zoom; motion detection; privacy masks; motorized zoom and focus (lens); dynamic ROI.
11)	Video Content Analysis:  Tampering/defocus, motion.
12)	Supported Protocols:  IPv4/IPv6, TCP, HTTP, HTTPS, RTSP, RTCP, RTP, RTMP, SMTP, SNMP v1/2c/3, UPnP, TLS/TTLS, HLS, ICMP, IGMP, LDAP, NTP, DHCP, FTP, DNS, DDNS, UDP, QoS, ARP, PPPoE, Bonjour, ONVIF S/G/Q/T.
** NOTE TO SPECIFIER **  Delete if not required.
G.	Analog Cameras:
** NOTE TO SPECIFIER **  Delete basis of design subparagraphs not required.
1.	Basis of Design:  V672B-W312MIR HD Analog Bullet Cameras as manufactured by Vicon Industries:
a.	Certifications:
1)	CE.
2)	FCC, Class A.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Analog Day/Night IR Bullet Camera:
1)	IR Illumination:
a)	For low or no light operation and maximum image resolution.
b)	Lens:  An integral, motorized 2.8 to 12 mm.
c)	Camera’s true wide dynamic range to improve detail in bright and low-light areas of the image.
2)	Resolution:  2 MP in AHD/TVI and 700 TVL in CVBS.
3)	Built-In Digital Noise Reduction (DNR):  To improve image quality in low-light environments.
4)	Privacy Masking:  The ability to mask up to 16 selected regions of the screen.
5)	Motion detection, backlight compensation and automatic white balance.
6)	Construction:  Aluminum and IP66 rated.
7)	Mounting:  Wall or ceiling.
a)	Adjustable:  Pan, 180 degrees; tilt from vertical, 90 degrees.
8)	Designed for easy installation and setup.
9)	Extensive Onscreen Display:  Menus allow set up of white balance, AGC, backlight compensation, exposure, privacy masks and many other functions.
10)	Accept UTC (up the coax) protocol.
11)	A PAL model shall be available.
e.	Camera and Optics Specifications:
1)	Image Device:  1/2.8 inch CMOS.
2)	Picture Elements:  1937(H) x 1097 (V).
3)	Scanning System:  16:9 progressive.
4)	Synchronization:  Internal.
5)	Shutter Speed:  Auto, Flicker, 1/30-1/30,000 sec manual.
6)	Horizontal Resolution:  AHD/TVI:  2 MP (1080p); CVBS:  700 TV lines.
7)	Sensitivity:  Color:  0. 03 lux, DSS off 0 fc (0 lux) with LEDs On.
8)	Video Output:  BNC 1 (TVI/AHD); BNC 2 (CVBS).
9)	S/N Ratio:  Greater than 52 dB (AGC off).
10)	IR LED/Sensor:  42 LEDs.
11)	IR Distance:  Up to 130 feet (40 m).
12)	Camera Control:  Joystick OSD; coaxial.
13)	Backlight Compensation:  WDR/BLC/HLC/Off.
14)	Automatic Gain Control (AGC):  1 to 10.
15)	Dynamic Range:  True WDR (120 dB)
16)	Digital Noise Reduction:  DNR (Low/Mid/High/Off).
17)	White Balance:  AWB Auto(Indoor)/Autoext (Outdoor)/Preset/Manual.
18)	Privacy Mask:  16 programmable zones.
19)	Day/Night:  Color/Black and White/Auto/External.
20)	Exposure:  DC  (ALC)/Manual (ELC).
21)	Focal Length:  2.8 to 12 mm, motorized.
22)	Field of View:  2.8 mm:  91 degrees H; 12 mm:  28 degrees H.
f.	Operational:
1)	Control Display:  On-screen, menu-driven system allowing full configuration of the camera.
2)	Lens Adjustment:  Motorized.
3)	Motion Detection:  4 areas. On/Off. Adjustable size and sensitivity.
4)	Titling:  On/Off, alphanumeric character set.
5)	Effects:  Flip/Mirror/Shading/Sharpness.
g.	Electrical Specifications:
1)	Input Voltage:  12 VDC plus or minus 10 percent or 24 VAC plus or minus 10 percent.
2)	Current:  0.63 A.
3)	Power Consumption:  7.5 W.
4)	Connectors:  
a)	Power:  2-pin connector.
b)	Video:  2  BNCs (1 for TVI/AHD, 1 for CVBS) on pendant cable.
c)	Spot monitor (for CVBS output).
h.	Environmental Specifications:
1)	Operating:  Outdoor rated:  
2)	Temperature:  14 to 122 degrees F (minus 10 to 50 degrees C)
3)	Humidity:  Up to 96 percent relative, non-condensing.
i.	Mechanical Specifications:
1)	Construction:  Aluminum. IP66 rated.
2)	Dimensions:
a)	Height:  3.9 inch (98.4 mm).
b)	Length with Mount:  11.8 inch (300 mm).
c)	Diameter:  3.4 inch (87 mm).
3)	Weight:  2.2 lbs (1.0 kg).
2.	Basis of Design:  V672D-W312MIR HD Analog Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:
1)	CE 
2)	FCC, Class A
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Analog Day/Night IR Dome Camera:
1)	Incorporate a camera and lens combination with a 2.8-12 mm motorized varifocal lens.
a)	Camera’s true wide dynamic range to improve detail in bright and low-light areas of the image.
b)	Contain 30 LEDs for use in no-light environments. 
c)	Illuminated distance with the LEDs on shall be 98 feet (30 m).
2)	Resolution:  2 MP in AHD/TVI and 700 TVL in CVBS.
3)	Built-In Digital Noise Reduction (DNR):  To improve image quality in low-light environments.
4)	Privacy Masking:  The ability to mask up to 16 selected regions of the screen.
5)	Motion detection, backlight compensation and automatic white balance.
6)	Construction:  PA 7 plastic with a high-impact polycarbonate plastic dome. Tamper-resistant screws.
a)	Rating:  IK10 and IP66.
b)	Mounting:  Wall or ceiling. 
7)	Adjustable:  Pan, 180 degrees; tilt from vertical, 90 degrees.
8)	Adjustable:  3-axis, pan, 360 degrees; tilt, 78 degrees from vertical, and rotation about its axis.
9)	Designed for easy installation and setup.
10)	Extensive Onscreen Display:  Menus allow set up of white balance, AGC, backlight compensation, exposure, privacy masks and many other functions.
11)	Accept UTC (up the coax) protocol.
12)	A PAL model shall be available.
e.	Camera and Optics Specifications:
1)	Image Device:  1/2.8 inch CMOS.
2)	Picture Elements:  1937(H) x 1097 (V).
3)	Scanning System:  16:9 progressive.
4)	Synchronization:  Internal.
5)	Shutter Speed:  Auto, Flicker, 1/30-1/30,000 sec manual.
6)	Horizontal Resolution:  AHD/TVI:  2 MP (1080p); CVBS:  700 TV lines.
7)	Sensitivity:  Color:  0. 03 lux, DSS off 0 fc (0 lux) with LEDs On.
8)	Video Output:  BNC 1 (TVI/AHD); BNC 2 (CVBS).
9)	S/N Ratio:  Greater than 52 dB (AGC off).
10)	IR LED/Sensor:  30 LEDs.
11)	IR Distance:  Up to 98 feet (30 m).
12)	Camera Control:  Joystick OSD; coaxial.
13)	Backlight Compensation:  WDR/BLC/HLC/Off.
14)	Automatic Gain Control (AGC):  1 to 10.
15)	Dynamic Range:  True WDR (120 dB)
16)	Digital Noise Reduction:  DNR (Low/Mid/High/Off).
17)	White Balance:  AWB Auto(Indoor)/Autoext (Outdoor)/Preset/Manual.
18)	Privacy Mask:  16 programmable zones.
19)	Day/Night:  Color/Black and White/Auto/External.
20)	Exposure:  DC  (ALC)/Manual (ELC).
21)	Focal Length:  2.8 to 12 mm, motorized.
22)	Field of View:  2.8 mm:  19.9 degrees H; 12 mm:  28.8 degrees H.
f.	Operational:
1)	Control Display:  On-screen, menu-driven system allowing full configuration of the camera.
2)	Lens Adjustment:  Motorized.
3)	Motion Detection:  4 areas. On/Off. Adjustable size and sensitivity.
4)	Titling:  On/Off, alphanumeric character set.
5)	Effects:  Flip/Mirror/Shading/Sharpness.
g.	Electrical Specifications:
1)	Input Voltage:  12 VDC plus or minus 10 percent or 24 VAC plus or minus 10 percent.
2)	Current:  0.60 A.
3)	Power Consumption:  7.2 W.
4)	Connectors:
a)	Power:  2-pin connector.
b)	Video:  2  BNCs (1 for TVI/AHD, 1 for CVBS) on pendant cable.
c)	Spot monitor (for CVBS output).
h.	Environmental Specifications:
1)	Operating:  Outdoor rated.
2)	Temperature:  14 to 122 degrees F (minus 10 to 50 degrees C).
3)	Humidity:  Up to 96 percent relative, non-condensing.
i.	Mechanical Specifications:
1)	Construction:  PA 7 plastic housing; high-impact polycarbonate plastic dome; tamper-resistant screws. IP66/IK10 rated.
2)	Dimensions:
a)	Height:  4.5 inch (114 mm).
b)	Housing Diameter:  5.65 inch (143.4 mm)
c)	Dome Diameter:  3.9 inch (99 mm)
3)	Weight:  1.16 lb (0.53 kg).
3.	Basis of Design:  V672V-W312MIR HD Analog Vandalproof Dome Cameras as manufactured by Vicon Industries:
a.	Certifications:
1)	CE.
2)	FCC, Class A.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Analog Day/Night IR Dome Camera:
1)	Incorporate a camera and lens combination with a 2.8-12 mm motorized varifocal lens.
a)	Camera’s true wide dynamic range to improve detail in bright and low-light areas of the image.
b)	Contain 30 LEDs for use in no-light environments.
c)	Illuminated distance with the LEDs on shall be 98 feet (30 m).
2)	Resolution:  2 MP in AHD/TVI and 700 TVL in CVBS.
3)	Built-In Digital Noise Reduction (DNR):  To improve image quality in low-light environments.
4)	Privacy Masking:  The ability to mask up to 16 selected regions of the screen.
5)	Motion detection, backlight compensation and automatic white balance.
6)	Construction:  Die-cast aluminum with high-impact polycarbonate plastic dome and tamper-resistant screws. 
a)	Rating:  IK10 and IP66.
b)	Mounting:  Wall or ceiling. 
7)	Adjustable:  3-axis, pan, 360 degrees; tilt, 78 degrees from vertical, and rotation about its axis.
8)	Designed for easy installation and setup.
9)	Extensive Onscreen Display:  Menus allow set up of white balance, AGC, backlight compensation, exposure, privacy masks and many other functions.
10)	Accept UTC (up the coax) protocol.
11)	A PAL model shall be available.
e.	Camera and Optics Specifications:
1)	Image Device:  1/2.8 inch CMOS.
2)	Picture Elements:  1937(H) x 1097 (V).
3)	Scanning System:  16:9 progressive.
4)	Synchronization:  Internal.
5)	Shutter Speed:  Auto, Flicker, 1/30-1/30,000 sec manual.
6)	Horizontal Resolution:  AHD/TVI:  2 MP (1080p); CVBS:  700 TV lines.
7)	Sensitivity:  Color:  0. 03 lux, DSS off 0 fc (0 lux) with LEDs On.
8)	Video Output:  BNC 1 (TVI/AHD); BNC 2 (CVBS).
9)	S/N Ratio:  Greater than 52 dB (AGC off).
10)	IR LED/Sensor:  30 LEDs.
11)	IR Distance:  Up to 98 feet (30 m).
12)	Camera Control:  Joystick OSD; coaxial.
13)	Backlight Compensation:  WDR/BLC/HLC/Off.
14)	Automatic Gain Control (AGC):  1 to 10.
15)	Dynamic Range:  True WDR (120 dB)
16)	Digital Noise Reduction:  DNR (Low/Mid/High/Off).
17)	White Balance:  AWB Auto(Indoor)/Autoext (Outdoor)/Preset/Manual.
18)	Privacy Mask:  16 programmable zones.
19)	Day/Night:  Color/Black and White/Auto/External.
20)	Exposure:  DC  (ALC)/Manual (ELC).
21)	Focal Length:  2.8 to 12 mm, motorized.
22)	Field of View:  2.8 mm:  94.2 degrees H; 12 mm:  26.2 degrees H.
f.	Operational:
1)	Control Display:  On-screen, menu-driven system allowing full configuration of the camera.
2)	Lens Adjustment:  Motorized.
3)	Motion Detection:  4 areas. On/Off. Adjustable size and sensitivity.
4)	Titling:  On/Off, alphanumeric character set.
5)	Effects:  Flip/Mirror/Shading/Sharpness.
g.	Electrical Specifications:
1)	Input Voltage:  12 VDC plus or minus 10 percent or 24 VAC plus or minus 10 percent.
2)	Current:  0.60 A.
3)	Power Consumption:  7.2 W.
4)	Connectors:  
a)	Power:  2-pin connector.
b)	Video:  2  BNCs (1 for TVI/AHD, 1 for CVBS) on pendant cable.
c)	Spot monitor (for CVBS output).
h.	Environmental Specifications:
1)	Operating:  Outdoor rated.
2)	Temperature:  14 to 122 degrees F (minus 10 to 50 degrees C).
3)	Humidity:  Up to 96 .percent relative, non-condensing.
i.	Mechanical Specifications:
1)	Construction:  Die-cast aluminum housing; high-impact polycarbonate plastic dome; tamper-resistant screws. IP66/IK10 rated.
2)	Dimensions:
a)	Height:  4.5 inch (114 mm).
b)	Housing Diameter:  5.88 inch (146.4 mm)
c)	Dome Diameter:  3.9 inch (99 mm)
3)	Weight:  1.7 lb (0.7 kg).
4.	Basis of Design:  V672-W-NL HD Analog Box Cameras as manufactured by Vicon Industries:
a.	Certifications:
1)	CE 
2)	FCC, Class A
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Analog Day/Night IR Dome Camera:
1)	Lightweight and compact, mountable in a variety of locations. Day/night type with ICR filter for low-light operation with maximum image resolution. 1/2.8 in. CMOS image device.
2)	The camera shall have a resolution of 2 MP in AHD/TVI and 700 TVL in CVBS. Built-in digital noise reduction (DNR) shall improve image quality in low-light environments.
3)	Privacy masking shall provide the ability to mask out up to 16 selected regions of the screen. 
4)	The camera shall provide motion detection, backlight compensation and automatic white balance.
5)	Construction:  Aluminum. A C/CS lens mount and an auto iris DIN connector. Mounting holes on bottom that fit a variety of mounts.
6)	Designed for easy installation and setup.
7)	Extensive Onscreen Display:  Menus allow set up of white balance, AGC, backlight compensation, exposure, privacy masks and many other functions.
8)	A PAL model shall be available.
e.	Camera and Optics Specifications:
1)	Image Device:  1/2.8 inch CMOS.
2)	Picture Elements:  1937(H) x 1097 (V).
3)	Scanning System:  16:9 progressive.
4)	Synchronization:  Internal.
5)	Shutter Speed:  Auto, Flicker, 1/30-1/30,000 sec manual.
6)	Horizontal Resolution:  AHD/TVI:  2 MP (1080p); CVBS:  700 TV lines.
7)	Sensitivity:  Color:  0. 03 lux, DSS off.
8)	Video Output:  BNC 1 (TVI/AHD); BNC 2 (CVBS).
9)	S/N Ratio:  Greater than 52 dB (AGC off).
10)	IR LED/Sensor:  30 LEDs.
11)	Camera Control:  OSD; coaxial.
12)	Backlight Compensation:  WDR/BLC/HLC/Off.
13)	Automatic Gain Control (AGC):  1 to 10.
14)	Dynamic Range:  True WDR (120 dB)
15)	Digital Noise Reduction:  DNR (Low/Mid/High/Off).
16)	White Balance:  AWB Auto(Indoor)/Autoext (Outdoor)/Preset/Manual.
17)	Privacy Mask:  16 programmable zones.
18)	Day/Night:  Color/Black and White/Auto/External.
19)	Exposure:  DC  (ALC)/Manual (ELC).
f.	Operational:
1)	Control Display:  On-screen, menu-driven system allowing full configuration of the camera.
2)	Lens Adjustment:  Motorized.
3)	Motion Detection:  4 areas. On/Off. Adjustable size and sensitivity.
4)	Titling:  On/Off, alphanumeric character set.
5)	Effects:  Flip/Mirror/Shading/Sharpness.
g.	Electrical Specifications:
1)	Input Voltage:  12 VDC plus or minus 10 percent or 24 VAC plus or minus 10 percent.
2)	Current:  0.25 A.
3)	Power Consumption:  3 W.
4)	Connectors:  
a)	Power:  2-pin connector.
b)	Video:  2 BNCs (1 for TVI/AHD, 1 for CVBS).
c)	C/CS lens mount.
h.	Environmental Specifications:
1)	Operating:  Outdoor rated.
2)	Temperature:  14 to 122 degrees F (minus 10 to 50 degrees C)
3)	Humidity:  Up to 96 .percent relative, non-condensing.
i.	Mechanical Specifications:
1)	Construction:  Aluminum.
2)	Dimensions:
a)	Height:  2.2 inch (56 mm) 
b)	Width:  2.6 inch (66 mm)
c)	Length:  4.7 inch (120 mm)
3)	Weight:  0.56 lbs (0.25 kg).
5.	Basis of Design:  V682-PTZ HD Analog PTZ Dome Camera as manufactured by Vicon Industries:
a.	Certifications:
1)	CE.
2)	FCC, Class A.
b.	Equipment and Materials:  Standard components regularly manufactured and used in the manufacturer’s system.
c.	Systems and Components:  Thoroughly tested and proven in actual use.
1)	Provided with the availability of a toll free 24- hour technical support phone number from the manufacturer. This no charge service shall be available to dealers and installers.
2)	Provided with an explicit 3-year manufacturer warranty.
d.	Analog Day/Night PTZ Dome Camera:
1)	Incorporate a camera and lens combination with a 4.7-94 mm motorized varifocal lens.
a)	Camera’s true wide dynamic range to improve detail in bright and low-light areas of the image.
2)	Resolution:  2 MP in AHD/TVI.
3)	Built-In Digital Noise Reduction (DNR):  To improve image quality in low-light environments.
4)	Privacy Masking:  The ability to mask up to 16 selected regions of the screen.
5)	Motion detection, backlight compensation and automatic white balance.
6)	Construction:  Aluminum base with high-impact polycarbonate plastic dome and tamper-resistant screws. 
a)	Rating:  IK10 and IP66.
b)	Mounting:  Wall or ceiling. 
7)	Designed for easy installation and setup.
8)	Extensive Onscreen Display:  Menus allow set up of white balance, AGC, backlight compensation, exposure, privacy masks and many other functions.
9)	Four alarm inputs shall be programmable for functional state (enabled or disabled); it shall be able to be set for Normally Open (NO) or Normally Closed (NC). Two alarm outputs shall be able to control external equipment; it shall be able to be set for Normally Open (NO) or Normally Closed (NC).
10.	There shall be 256 individual programmable preset positions available. Each preset shall be able to have an individual title and shall be adjustable for pan and tilt speed and manual or auto focus.
11.	There shall be 8 tours available with can consist of up to 40 presets, patterns, scans or other tours. Each tour and pattern shall be able to have an individual title and shall be adjustable for pan, tilt and zoom speed and dwell time. Tours shall be able to be programmed to repeat. There shall be 8 patterns available.
12.	Pan and tilt functions shall be programmable. Maximum manual pan and tilt speeds shall be programmable. Maximum pan speed shall be 380 degrees/sec and maximum tilt speed shall be 380 degrees/sec. Pan and tilt speeds shall also be scalable to the zoom setting. The pan range shall be 360 degree continuous and tilt range shall be 180 degrees (0 to 180 degrees).
10)	Accept UTC (up the coax) protocol.
e.	Camera and Optics Specifications:
1)	Image Device:  1/2.8 inch CMOS.
2)	Resolution:  1080p HD-TVI or AHD.
3)	Scanning System:  Progressive.
4)	Shutter Speed:  Auto, 1/30,000 – x8 sec manual @30/25 fps.
5)	Sensitivity:  Color:  0. 35 lux, B&W: 0.013 lux.
6)	Video Output:  BNC.
7)	Camera Control:  Joystick OSD; coaxial.
8)	Backlight Compensation:  WDR/BLC/HLC/Off.
9)	Dynamic Range:  True WDR (120 dB)
10)	Digital Noise Reduction:  DNR (Low/Mid/High/Off).
11)	White Balance:  AWB Auto, Outdoor, Incandescent, Fluorescent, Manual.
12)	Privacy Mask:  16 programmable zones.
13)	Day/Night:  Color/Black and White/Auto/External.
14)	Exposure:  DC  ALC)/Manual (ELC).
15)	Focal Length:  4.7 to 94 mm, motorized.
16)	Field of View:  55.5 degrees H; 3 degrees H.
f.	Operational:
1)	Range: Pan: 360° continuous; Tilt 0-180°. Speed: Pan: 380°/sec (preset); Tilt 380°/sec (preset).
2)	Control Display:  On-screen, menu-driven system allowing full configuration of the camera.
3)	Lens Adjustment:  Motorized.
4)	Motion Detection:  On/Off. Adjustable size and sensitivity.
5)	Titling:  On/Off, alphanumeric character set.
6)	Effects:  Flip.
g.	Electrical Specifications:
1)	Input Voltage:  12 VDC or 24 VAC; Heater/Fan: 24 VAC.
2)	Current:  1 A; Heater/Fan: 1.7A.
3)	Power Consumption:  12 W; Heater/Fan: 45 W.
4)	Connectors:  
a)	Power:  3-pin connector.
b)	Heater/fan: 3-pin connector.
c)	Alarm Input/Output: terminal block
d)	Video:  BNC jack.
e)	Video Composite Output: BNC jack
f)	Control: RS-485
h.	Environmental Specifications:
1)	Operating:  Outdoor rated.
2)	Temperature:  minus 58 to 131 degrees F (minus 50 to 55 degrees C).
3)	Humidity:  Up to 90 .percent relative, non-condensing.
i.	Mechanical Specifications:
1)	Construction:  Die-cast aluminum housing; high-impact polycarbonate plastic dome; tamper-resistant screws. IP66/IK10 rated.
2)	Dimensions:
a)	Height:  8.4 inch (213 mm).
b)	Housing Diameter:  7.3 inch (120 mm)
c)	Dome Diameter:  4.7 inch (120 mm)
3)	Weight:  5.1 lb (2.3 kg).

H.	Manufacturer requires the use of uninterruptible power supply systems (UPS) to prevent voltage fluctuations that can affect operation and cause damage to the equipment. Failure to comply voids the warranty.
END OF SECTION